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	Name of Substance
	Cement
	COSHH

Reference 
	C015

	Supplied By
	n/a
	Date of 
Assessment
	25/07/25

	Persons at Risk
	Staff
       X
	Public          X
	Young/Pregnant

Workers               X
	Review Date
	24/07/25

	
	Visitors       X
	Contractor   X
	
	
	

	Description of Substance
	Cements are used in industrial installations to manufacture / formulate hydraulic binders for building and construction work, such as ready-mixed concrete, mortars, renders, grouts, plasters as well as precast concrete.
	Method of use
	Common cements and cement containing mixtures (hydraulic binders) are used industrially, by professionals as well as by consumers in building and construction work, indoor and outdoor. The identified uses of cements and cement containing mixtures cover the dry products and the products in a wet suspension (paste).


	

	Hazards Identification and PPE

	Routes of Entry
	Personal Protective Equipment (Tick Required Boxes)
	Tick here for none
 FORMCHECKBOX 


	Inhalation
X
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	Absorption
X
	
	
	
	
	
	
	

	Ingestion
X
	
	
	
	
	
	
	

	Location
	Hand Protection
	Protective clothing
	Protective Footwear
	Safety Glasses
	Face Shield
	Face Mask
	Respirator

	     
	X
	
	X
	X
	
	
	X

	

	Risk Phrases

Safety Phrases
	Workplace exposure Limits (WEL) 

	Portland Cement Clinker Dust & Flue dust from production of cement clinker:

H318 Causes serious eye damage

H315 Causes skin irritation

H317 May cause an allergic skin reaction

H335 May cause respiratory irritation
	Respirable Dust Long Term Exp. Limit (8 Hours):

4 mg/m3 

N.B: Industrial use of cement for the formulation of hydraulic building and construction materials - Duration is not restricted (up to 480 minutes per shift, 5 shifts a week)



	

	Frequency & Duration of Exposure

	Amount Used

Small (Millilitres)
 FORMCHECKBOX 

Medium Litres

 FORMCHECKBOX 

Large Cubic Metres
 X
	How many times per day

1 – 5

 X
5 – 10

 FORMCHECKBOX 

More than 10
 FORMCHECKBOX 

	Duration

1 – 5 Minutes

 FORMCHECKBOX 

6 – 30 Minutes
 FORMCHECKBOX 

31 – 60 Minutes
 X
1 Hour & Above
 FORMCHECKBOX 


	SUBSTANCE PROPERTIES (Tick all that apply)
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	Oxidising
	Explosive
	Flammable
Highly Flammable
	Toxic
	Harmful or Irritant
	Corrosive
	Carcinogenic
Mutagenic
	Dangerous for environment

	
	
	
	X
	X
	
	
	


	GHS SUBSTANCE PROPERTIES
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	Oxidising
	Explosive
	(Extremely) Flammable
	Toxic
	Harmful
	Corrosive
	Human Health
	Dangerous for environment
	Gas under pressure

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	X
	X
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 



	Control Measures

	General Precautions
	First Aid Measures

	Keep out of reach of children.
Wear protective gloves/protective clothing/eye

protection/face protection.
Do not sweep. Use dry clean up methods such as vacuum clean-up or vacuum extraction, which do not cause airborne dispersion.
Do not handle or store near food and beverages or smoking materials. 
In dusty environment, wear dust mask and protective goggles. Use protective gloves to avoid

skin contact.

During work avoid kneeling in fresh mortar or concrete wherever possible. If kneeling is absolutely necessary then appropriate waterproof personal protective equipment must be worn. 
Do not eat, drink or smoke when working with cement to avoid contact with skin or mouth. 
Before starting to work with cement, apply a barrier cream and reapply it at regular intervals. 
Immediately after working with cement or cement containing materials, workers should wash or shower or use skin moisturisers.
Remove contaminated clothing, footwear, watches, etc. and clean thoroughly before re-using them.
	Inhalation

Avoid breathing dust. IF INHALED: Remove victim to fresh

air and keep at rest in a position comfortable for breathing.

Call a poison centre or doctor/physician if you feel

unwell.
Ingestion

Do not induce vomiting. If the person is conscious, wash out mouth with water and give plenty of water to drink. Get immediate medical attention or contact the anti-poison centre.
Skin Contact

IF ON SKIN: Wash with plenty of soap and water. If skin

irritation or rash occurs: Get medical advice/attention.
Eye Contact

IF IN EYES: Rinse cautiously with water for several minutes.

Remove contact lenses, if present and easy to do. Continue

rinsing. Immediately call a poison centre or

doctor/physician.     

	
	

	Further Controls Required
	Responsibility
	By When
	Date Done

	N/A
	     
	     
	     

	

	Spillage Procedure
	Fire Prevention

	Collect the spillage in a dry state if possible.


Dry cement:
Use clean up methods such as vacuum clean-up or vacuum extraction (Industrial portable units, equipped with high efficiency air filters (EPA and HEPA filters, EN 1822-1:2009) or equivalent technique) which do not cause airborne dispersion. Never use compressed air. Alternatively, wipe-up the dust by mopping, wet brushing or by using water sprays or hoses (fine mist to avoid that the dust becomes airborne) and remove slurry. If not possible, remove

by slurrying with water (see wet cement). When wet cleaning or vacuum cleaning is not possible and only dry cleaning with brushes can be done, ensure that the workers wear the appropriate personal protective equipment and prevent dust from spreading. Avoid inhalation of cement and contact with skin. Place spilled materials into a container. Solidify before disposal.

Wet cement:
Clean up wet cement and place in a container. Allow material to dry and solidify before disposal.
	Cement poses no fire-related hazards. 
Cements are non-combustible and non-explosive and will not facilitate or sustain the combustion of other materials.

	
	

	Handling and Storage
	Disposal Considerations

	Do not eat, drink or smoke when working with cement to avoid contact with skin or mouth. 
Packed products should be stored in unopened bags clear of the ground in cool, dry conditions and protected from excessive draught in order to avoid degradation of quality. Bags should be stacked in a stable manner.
Do not use aluminium containers for the storage or transport of wet cement containing mixtures due to incompatibility of the materials.
	Dispose of waste and residues in accordance with local authority requirements. 
Pick up dry unused residue or dry spillage as is. Mark the containers. Possibly reuse depending upon shelf life considerations and the requirement to avoid dust exposure. In case of disposal, harden with water and dispose.

Dispose of according to the local legislation. Avoid entry into the sewage water system.
Dispose of the hardened product as concrete waste. 
Due to the inertisation, concrete waste is not a dangerous waste.

	


	COSHH Assessment Comments

	     


	Assessor Summary
	
	YES/NO
	Further action

	1.
Has the assessment considered all factors 
pertinent to the use of the substance?  If NO 
please give 
details of further action required
	YES
	     

	2.
Has the assessment considered the 
practicability of preventing exposure?  If NO 
please give 
details of further action required
	YES
	     

	3.
Has the assessment considered the steps to 
be taken to achieve and maintain adequate 
control of exposure where prevention is not 
reasonably practicable?  If NO please give 
details of further action required
	YES
	     

	4.
Has the assessment considered the need for 
monitoring exposure to the substance  If NO 
please give details of further action required
	YES
	     

	5.
Has the assessment identified all action 
required to comply with regulations  If NO 
please give details of further action required
	YES
	     

	

	COSHH Assessment
	Please tick
	

	

	The task is safe to be carried out with current control procedures.
	X
	Tick if no further action required

	The task is safe to be carried out subject to actions listed
	     
	Tick if use of the substance is not causing significant problems but requires some action to bring it within COSHH guidelines, Action should be prioritised and specific dates set for completion

	Task/Substance is Unsafe, significant non-compliance with Health & Safety standards
	     
	Tick if the task or substance has potential to cause significant problems to users, use of substance to be discontinued until problems have been rectified

	     
The Task/process should be re-assessed on a regular basis either annually, or if there are significant changes to the task or process or if there is a significant change in personnel who carry it out it e.g. young/inexperienced workers, pregnancy, workers with pre-existing conditions such as asthma, dermatitis etc

Signed Assessor





Date     
……………………………………………………………………
………………………………………

This Assessment has been discussed with the user their line manager and action agreed

Signed:
User
     



Line Manager 
     


Date     
……………………………………….
……………………………….……

……………..
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