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	Name of Substance
	Diall (B&Q) White Spirit
	COSHH

Reference 
	C020     

	Supplied By
	B&Q
	Date of 
Assessment
	25/07/25

	Persons at Risk
	Staff
       X
	Public          FORMCHECKBOX 

	Young/Pregnant

Workers                FORMCHECKBOX 

	Review Date
	24/07/26

	
	Visitors       X 
	Contractor   X
	
	
	

	Description of Substance
	General degreasing solvent. 
	Method of use
	Paint brush cleaner Paint thinner

	

	Hazards Identification and PPE

	Routes of Entry
	Personal Protective Equipment (Tick Required Boxes)
	Tick here for none
 FORMCHECKBOX 


	Inhalation
X
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	Absorption
X
	
	
	
	
	
	
	

	Ingestion
X
	
	
	
	
	
	
	

	Location
	Hand Protection
	Protective clothing
	Protective Footwear
	Safety Glasses
	Face Shield
	Face Mask
	Respirator

	     
	X
	X
	
	X
	
	
	X

	

	Risk Phrases

Safety Phrases
	Workplace exposure Limits (WEL) 

	H226 Flammable liquid and vapour.

H304 May be fatal if swallowed and enters airways.

H336 May cause drowsiness or dizziness.

H372 Causes damage to organs through prolonged or repeated exposure.

H411 Toxic to aquatic life with long lasting effects
	Hydrocarbons, C9-C12, n-alkanes, isoalkanes, cyclics, aromatics (2-25%) 100%

Long-term exposure limit (8-hour TWA): 350 mg/m³ vapour

	

	Frequency & Duration of Exposure

	Amount Used

Small (Millilitres)
 X
Medium (Litres)
 FORMCHECKBOX 

Large (Cubic Metres)
 FORMCHECKBOX 

	How many times per day

1 – 5

 X
5 – 10

 FORMCHECKBOX 

More than 10
 FORMCHECKBOX 

	Duration

1 – 5 Minutes

 X
6 – 30 Minutes
 FORMCHECKBOX 

31 – 60 Minutes
 FORMCHECKBOX 

1 Hour & Above
 FORMCHECKBOX 


	SUBSTANCE PROPERTIES (Tick all that apply)
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	Oxidising
	Explosive
	Flammable
Highly Flammable
	Toxic
	Harmful or Irritant
	Corrosive
	Carcinogenic
Mutagenic
	Dangerous for environment

	
	X
	X
	
	X
	
	
	X


	GHS SUBSTANCE PROPERTIES
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	Oxidising
	Explosive
	(Extremely) Flammable
	Toxic
	Harmful
	Corrosive
	Human Health
	Dangerous for environment
	Gas under pressure

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	X
	 FORMCHECKBOX 

	X
	 FORMCHECKBOX 

	X
	X
	 FORMCHECKBOX 



	Control Measures

	General Precautions
	First Aid Measures

	Persons with impaired lung function should not handle this product. Pregnant or breastfeeding women should not work with this product if there is any risk of exposure. Wash hands thoroughly after handling. Wash promptly if skin becomes contaminated. Care should be taken to avoid contact with contaminants when removing contaminated clothing. Promptly remove any clothing that becomes wet or contaminated. Remove contaminated clothing and protective equipment before entering eating areas. Change work clothing daily before leaving

workplace. Wash contaminated clothing before reuse. Wash at the end of each work shift and

before eating, smoking and using the toilet. Use appropriate hand lotion to prevent defatting

and cracking of skin. Do not eat, drink or smoke when using this product
This product is not to be used under conditions of poor ventilation. This product must not be

handled in a confined space without adequate ventilation. Mechanical ventilation or local

exhaust ventilation may be required. In case of insufficient ventilation, wear suitable respiratory equipment. Avoid inhalation of vapours and spray/mists. Use explosion-proof electrical, ventilating and lighting equipment. Personal protective equipment should only be used if worker exposure cannot be controlled adequately by the engineering control measures.
Wear EN 166 approved chemical safety goggles where eye exposure is reasonably probable.

Chemical-resistant, impervious gloves complying with an approved standard should be worn if

a risk assessment indicates skin contact is possible.
Wear appropriate clothing to prevent any possibility of liquid contact and repeated or prolonged vapour contact.
	General information - Remove affected person from source of contamination. IN CASE OF SERIOUS OR PERSISTENT CONDITIONS, CALL A DOCTOR OR THE NHS 111 SERVICE.
Inhalation – Move the exposed person to fresh air at once. Get medical attention. Provide rest, warmth and fresh air. When breathing is difficult, properly trained personnel may assist affected person by administering oxygen.

Ingestion – DO NOT INDUCE VOMITING! NEVER MAKE AN UNCONSCIOUS PERSON VOMIT OR DRINK FLUIDS! If vomiting occurs, keep head low so that stomach content doesn't get into the lungs. Get medical attention immediately! Provide rest, warmth and fresh air.

Skin contact – Remove contaminated clothing. Wash the skin immediately with soap and water. Get medical attention promptly if symptoms occur after washing.

Eye contact –Rinse immediately with plenty of water. Remove contact lenses, if present and easy to do. Continue rinsing. Get medical attention if symptoms are severe or persist after washing.     

	
	

	Further Controls Required
	Responsibility
	By When
	Date Done

	     N/A
	     
	     
	     

	

	Spillage Procedure
	Fire Prevention

	Evacuate area. Keep unnecessary and unprotected personnel away from the spillage. No smoking, sparks, flames or other sources of ignition near spillage. Do not touch or walk into spilled material. Do not enter storage areas or confined spaces unless adequately ventilated.

Wear suitable protective equipment, including gloves, goggles/face shield, respirator, boots,

clothing or apron, as appropriate. Take precautionary measures against static discharges.

Take care as floors and other surfaces may become slippery.
	Extinguish with alcohol-resistant foam, carbon dioxide, dry powder or water fog.
Do not use water jet as an extinguisher, as this will spread the fire.
Vapours are heavier than air and may spread near ground and travel a considerable distance to a source of ignition and flash back.

	
	

	Handling and Storage
	Disposal Considerations

	Avoid contact with skin and eyes. Keep away from heat, sparks and open flame. Eliminate all

sources of ignition. Use explosion proof electric equipment. Storage tanks and other containers must be grounded. Wear full protective clothing for prolonged exposure and/or high concentrations. 
Contaminated clothing and shoes must be discarded. Contaminated rags and cloths must be put in fireproof containers for disposal. Ventilate well, avoid breathing vapours.
Use approved respirator if air contamination is above accepted level. Avoid spilling and release to the environment such as drains and watercourses.
Store in tightly-closed, original container in a dry, cool and well-ventilated place. Keep container tightly sealed when not in use. Keep locked up and out of the reach of children. Store in a demarcated bunded area to prevent release to drains and/or watercourses. Keep away from heat, hot surfaces, sparks, open flames and other ignition sources. No smoking. Avoid contact with oxidising agents. Keep away from food, drink and animal feeding stuffs. Use containers made of the following materials: Carbon steel. Glass. Mild steel. Stainless steel. High-density polyethylene (HDPE) Polyethylene terephthalate (PET).
	The generation of waste should be minimised or avoided wherever possible. Disposal of this product, process solutions, residues and by-products should at all times comply with the

requirements of environmental protection and waste disposal legislation and any local authority requirements. 
External recovery, treatment, recycling and disposal of waste should comply with all applicable local and/or national regulations. Waste material and any included combustible absorbent and containers should be suitable for incineration at an approved facility. This material and its container must be disposed of as hazardous waste. Waste packaging should be collected for reuse or recycling. The packaging must be empty (drop-free when inverted). When handling waste, the safety precautions applying to handling of the product should be considered.
Waste, residues, empty containers, discarded work clothes and contaminated cleaning materials should be collected in designated containers, labelled with their contents. Label the

containers containing waste and contaminated materials and remove from the area as soon as possible. Dispose of waste to licensed waste disposal site in accordance with the

requirements of the local Waste Disposal Authority. Waste material and any included combustible absorbent and containers should be suitable for incineration at an approved

facility. This material and its container must be disposed of as hazardous waste.

	


	Assessor Summary
	
	YES/NO
	Further action

	1.
Has the assessment considered all factors 
pertinent to the use of the substance?  If NO 
please give 
details of further action required
	YES
	     

	2.
Has the assessment considered the 
practicability of preventing exposure?  If NO 
please give 
details of further action required
	YES
	     

	3.
Has the assessment considered the steps to 
be taken to achieve and maintain adequate 
control of exposure where prevention is not 
reasonably practicable?  If NO please give 
details of further action required
	    YES 
	     

	4.
Has the assessment considered the need for 
monitoring exposure to the substance  If NO 
please give details of further action required
	YES  
	     

	5.
Has the assessment identified all action 
required to comply with regulations  If NO 
please give details of further action required
	YES   
	     

	

	COSHH Assessment
	Please tick
	

	

	The task is safe to be carried out with current control procedures.
	X
	Tick if no further action required

	The task is safe to be carried out subject to actions listed
	     
	Tick if use of the substance is not causing significant problems but requires some action to bring it within COSHH guidelines, Action should be prioritised and specific dates set for completion

	Task/Substance is Unsafe, significant non-compliance with Health & Safety standards
	     
	Tick if the task or substance has potential to cause significant problems to users, use of substance to be discontinued until problems have been rectified

	     
The Task/process should be re-assessed on a regular basis either annually, or if there are significant changes to the task or process or if there is a significant change in personnel who carry it out it e.g. young/inexperienced workers, pregnancy, workers with pre existing conditions such as asthma, dermatitis etc

Signed:  Assessor





Date     
……………………………………………………………………
………………………………………

This Assessment has been discussed with the user their line manager and action agreed

Signed:
User
     



Line Manager 
     


           Date     
……………………………………….
……………………………….……

……………..
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