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	Name of Substance
	Super Flow 30 - Powder
	COSHH

Reference 
	C023

	Supplied By
	Tillemaster
	Date of 
Assessment
	25/07/25

	Persons at Risk
	Staff
       X
	Public          FORMCHECKBOX 

	Young/Pregnant

Workers                FORMCHECKBOX 

	Review Date
	24/07/26

	
	Visitors       X
	Contractor   X
	
	
	

	Description of Substance
	Cement based self levelling underlayment
	Method of use
	Shake the bottle of liquid polymer and pour into a suitable clean mixing vessel. Add the powder component slowly whilst mixing for 2 minutes until a smooth and lump free consistency is obtained. Once mixed do not add further polymer liquid or water. Pour a small quantity onto the prepared surface and trowel down lightly to a depth between 2mm and 15mm.

	

	Hazards Identification and PPE

	Routes of Entry
	Personal Protective Equipment (Tick Required Boxes)
	Tick here for none
 FORMCHECKBOX 


	Inhalation
X
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	Absorption
X
	
	
	
	
	
	
	

	Ingestion
X
	
	
	
	
	
	
	

	Location
	Hand Protection
	Protective clothing
	Protective Footwear
	Safety Glasses
	Face Shield
	Face Mask
	Respirator

	     
	X
	
	
	X
	
	X
	

	

	Risk Phrases

Safety Phrases
	Occupational Exposure Standard (OES)
	Maximum Exposure Limits (MEL)
	Workplace exposure Limits (WEL) 

	N/A     
	N/A
	N/A
	N/A

	

	Frequency & Duration of Exposure

	Amount Used

Small (Millilitres)
 FORMCHECKBOX 

Medium Litres

 X
Large Cubic Metres
 FORMCHECKBOX 

	How many times per day

1 – 5

 X
5 – 10

 FORMCHECKBOX 

More than 10
 FORMCHECKBOX 

	Duration

1 – 5 Minutes

 FORMCHECKBOX 

6 – 30 Minutes
 FORMCHECKBOX 

31 – 60 Minutes
 FORMCHECKBOX 

1 Hour & Above
 X

	SUBSTANCE PROPERTIES (Tick all that apply)
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	Oxidising
	Explosive
	Flammable
Highly Flammable
	Toxic
	Harmful or Irritant
	Corrosive
	Carcinogenic
Mutagenic
	Dangerous for environment

	
	
	
	
	
	
	
	


	GHS SUBSTANCE PROPERTIES
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	Oxidising
	Explosive
	(Extremely) Flammable
	Toxic
	Harmful
	Corrosive
	Human Health
	Dangerous for environment
	Gas under pressure

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 



	Control Measures

	General Precautions
	First Aid Measures

	No Significant Hazard. 
Appropriate engineering controls - Ensure adequate ventilation of the working area.

Individual protection measures - Appropriate respiratory protection. 
Wear suitable gloves and eye/face protection.

Eye / face protection - Approved safety goggles. 
Skin protection – Hand protection Nitrile rubber gloves.
Respiratory protection Wear - Suitable respiratory equipment.
	Inhalation - Move the exposed person to fresh air.
Eye contact -  Irritating to eyes. Rinse immediately with plenty of water for 15 minutes holding the eyelids open. 

Skin contact -  Irritating to skin. Wash off immediately with plenty of soap and water. Remove contaminated clothing.

Ingestion -  Rinse mouth thoroughly. DO NOT INDUCE VOMITING

	
	

	Further Controls Required
	Responsibility
	By When
	Date Done

	N/A
	     
	     
	     

	

	Spillage Procedure
	Fire Prevention

	Avoid formation of dust. Avoid contact with skin and eyes. Use appropriate personal protective equipment.
Do not allow product to enter drains. 
Sweep up. Transfer to suitable, labelled containers for disposal. 

	Use extinguishing media appropriate to the surrounding fire conditions. Product itself is non-combustible. Only the packaging materials can catch fire. The extinguishing media normally used are sufficient.

	
	

	Handling and Storage
	Disposal Considerations

	Avoid contact with eyes and skin. Ensure adequate ventilation of the working area. Adopt best Manual Handling considerations when handling, carrying and dispensing. Avoid formation of dust. Wear suitable protective equipment.
	Dispose of in compliance with all local and national regulations.

	


	COSHH Assessment Comments

	     


	Assessor Summary
	
	YES/NO
	Further action

	1.
Has the assessment considered all factors 
pertinent to the use of the substance?  If NO 
please give 
details of further action required
	YES
	     

	2.
Has the assessment considered the 
practicability of preventing exposure?  If NO 
please give 
details of further action required
	YES
	     

	3.
Has the assessment considered the steps to 
be taken to achieve and maintain adequate 
control of exposure where prevention is not 
reasonably practicable?  If NO please give 
details of further action required
	YES
	     

	4.
Has the assessment considered the need for 
monitoring exposure to the substance  If NO 
please give details of further action required
	YES
	     

	5.
Has the assessment identified all action 
required to comply with regulations  If NO 
please give details of further action required
	YES
	     


	

	COSHH Assessment
	Please tick
	

	

	The task is safe to be carried out with current control procedures.
	X
	Tick if no further action required

	The task is safe to be carried out subject to actions listed
	     
	Tick if use of the substance is not causing significant problems but requires some action to bring it within COSHH guidelines, Action should be prioritised and specific dates set for completion

	Task/Substance is Unsafe, significant non-compliance with Health & Safety standards
	     
	Tick if the task or substance has potential to cause significant problems to users, use of substance to be discontinued until problems have been rectified

	     
The Task/process should be re-assessed on a regular basis either annually, or if there are significant changes to the task or process or if there is a significant change in personnel who carry it out it e.g. young/inexperienced workers, pregnancy, workers with pre existing conditions such as asthma, dermatitis etc

Signed Assessor





Date     
……………………………………………………………………
………………………………………

This Assessment has been discussed with the user their line manager and action agreed

Signed:
User
     



Line Manager 
     


Date     
……………………………………….
……………………………….……

……………..
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