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	Name of Substance
	ALTRO CRETE SLIP RESISTANT HARDENER
	COSHH

Reference 
	C027

	Supplied By
	Altro Resin Systems Ltd
	Date of 
Assessment
	25/07/25

	Persons at Risk
	Staff
       X
	Public          X
	Young/Pregnant

Workers                FORMCHECKBOX 

	Review Date
	24/07/26

	
	Visitors       X
	Contractor   X
	
	
	

	Description of Substance
	PU Hardeners- Industrial flooring, hardener component for polyurethane system
	Method of use
	Used in conjunction with Altro Crete Polyeurathane Flooring System

	

	Hazards Identification and PPE

	Routes of Entry
	Personal Protective Equipment (Tick Required Boxes)
	Tick here for none
 FORMCHECKBOX 


	Inhalation
X
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	Absorption
X
	
	
	
	
	
	
	

	Ingestion
X
	
	
	
	
	
	
	

	Location
	Hand Protection
	Protective clothing
	Protective Footwear
	Safety Glasses
	Face Shield
	Face Mask
	Respirator

	     
	X
	X
	
	X
	
	
	X

	

	Risk Phrases

Safety Phrases
	Workplace exposure Limits (WEL) 

	H315 Causes skin irritation.

H317 May cause an allergic skin reaction.

H319 Causes serious eye irritation.

H332 Harmful if inhaled.

H334 May cause allergy or asthma symptoms or breathing difficulties if inhaled.

H335 May cause respiratory irritation.

H351 Suspected of causing cancer.

H373 May cause damage to organs through prolonged or repeated exposure.     
	METHYLENEDIPHENYL DIISOCYANATE

Long-term exposure limit (8-hour TWA): WEL 0.02 mg/m3 
Short-term exposure limit (15-minute): WEL 0.07 mg/m3

DIPHENYLMETHANEDIISOCYANATE -Isomers & homologues

Long-term exposure limit (8-hour TWA): WEL 0.02 mg/m3
Short-term exposure limit (15-minute): WEL 0.07 mg/m3


	

	Frequency & Duration of Exposure

	Amount Used

Small (Millilitres)
 FORMCHECKBOX 

Medium Litres

 X
Large Cubic Metres
 FORMCHECKBOX 

	How many times per day

1 – 5

 X
5 – 10

 FORMCHECKBOX 

More than 10
 FORMCHECKBOX 

	Duration

1 – 5 Minutes

 FORMCHECKBOX 

6 – 30 Minutes            X
31 – 60 Minutes
 FORMCHECKBOX 

1 Hour & Above
 FORMCHECKBOX 


	SUBSTANCE PROPERTIES (Tick all that apply)
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	Oxidising
	Explosive
	Flammable
Highly Flammable
	Toxic
	Harmful or Irritant
	Corrosive
	Carcinogenic
Mutagenic
	Dangerous for environment

	
	
	
	
	X
	
	
	


	GHS SUBSTANCE PROPERTIES
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	Oxidising
	Explosive
	(Extremely) Flammable
	Toxic
	Harmful
	Corrosive
	Human Health
	Dangerous for environment
	Gas under pressure

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	X
	 FORMCHECKBOX 

	X
	 FORMCHECKBOX 

	 FORMCHECKBOX 



	Control Measures

	General Precautions
	First Aid Measures

	RESPIRATORY PROTECTION

Respiratory protection in case of vapour/aerosol release: Combination filter for gases/ vapours of organic compounds and solid liquid particles. (f.e. EN 14387 Type A-P2).
EYE PROTECTION
Safety glasses with side-shields.

HAND PROTECTION

Nitrile gloves. Butyl gloves. PVC gloves.

Wear protective clothing.

Ensure there is sufficient ventilation of the area. 
	AFTER INHALATION

Remove casualty from exposure ensuring one's own safety whilst doing so. Consult a doctor.

AFTER SKIN CONTACT

Wash immediately with plenty of soap and water.


AFTER EYE CONTACT
Bathe the eye with running water for 15 minutes. Transfer to hospital for specialist examination

AFTER INGESTION
Wash out mouth with water. If conscious, give half a litre of water to drink immediately. Consult a doctor.     

	
	

	Further Controls Required
	Responsibility
	By When
	Date Done

	N/A
	     
	     
	     

	

	Spillage Procedure
	Fire Prevention

	Ventilate the area to dispel residual vapours.
Do not discharge into drains or rivers. Do not discharge into subsoil/soil.
Take up with absorbent material (eg. sand, Kieselguhr, universal binder). Transfer to a

closable, labelled salvage container for disposal by an appropriate method.
	Stable under normal conditions.

Suitable extinguishing media is Dry chemical powder. Carbon dioxide. Alcohol resistant foam. Water spray.
In combustion emits toxic fumes of carbon dioxide / carbon monoxide. In combustion emits.
toxic fumes of hydrogen cyanide. In combustion emits toxic fumes of nitrogen oxides.
Special protective equipment for firefighters:
Wear self-contained breathing apparatus. Wear protective clothing to prevent contact with skin and eyes.

	Handling and Storage
	Disposal Considerations

	Store in cool, well ventilated area. Avoid contact with water or humidity. Keep container tightly closed. If moisture enters isocyanate containers, CO2 forms and pressure builds up. Protect from temperatures below 20°C and above 35°C.
	Do not discharge into drains or rivers. Contain the spillage using bunding.
Cured Material may be disposed of as plastic waste, uncured material and containers must be disposed of in accordance to local council regulations.

	


	Assessor Summary
	
	YES/NO
	Further action

	1.
Has the assessment considered all factors 
pertinent to the use of the substance?  If NO 
please give 
details of further action required
	YES
	     

	2.
Has the assessment considered the 
practicability of preventing exposure?  If NO 
please give 
details of further action required
	YES
	     

	3.
Has the assessment considered the steps to 
be taken to achieve and maintain adequate 
control of exposure where prevention is not 
reasonably practicable?  If NO please give 
details of further action required
	YES
	     

	4.
Has the assessment considered the need for 
monitoring exposure to the substance  If NO 
please give details of further action required
	YES
	     

	5.
Has the assessment identified all action 
required to comply with regulations  If NO 
please give details of further action required
	YES
	     

	

	COSHH Assessment
	Please tick
	

	

	The task is safe to be carried out with current control procedures.
	X
	Tick if no further action required

	The task is safe to be carried out subject to actions listed
	     
	Tick if use of the substance is not causing significant problems but requires some action to bring it within COSHH guidelines, Action should be prioritised and specific dates set for completion

	Task/Substance is Unsafe, significant non-compliance with Health & Safety standards
	     
	Tick if the task or substance has potential to cause significant problems to users, use of substance to be discontinued until problems have been rectified
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