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	Name of Substance
	Remmers Crete RT (Hardener Component)
	COSHH

Reference 
	C030

	Supplied By
	Remmers Baustofftechnik GmbH
	Date of 
Assessment
	25/07/25

	Persons at Risk
	Staff
       X
	Public          X
	Young/Pregnant

Workers                FORMCHECKBOX 

	Review Date
	24/07/26

	
	Visitors       X
	Contractor   X
	
	
	

	Description of Substance
	Hardener Component part of a 3-component polyurethane screed system.
	Method of use
	Water dispersed polyurethane resin system combined with graded silica aggregates.

	

	Hazards Identification and PPE

	Routes of Entry
	Personal Protective Equipment (Tick Required Boxes)
	Tick here for none
 FORMCHECKBOX 


	Inhalation
X
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	Absorption
X
	
	
	
	
	
	
	

	Ingestion
X
	
	
	
	
	
	
	

	Location
	Hand Protection
	Protective clothing
	Protective Footwear
	Safety Glasses
	Face Shield
	Face Mask
	Respirator

	     
	X
	X
	
	X
Tightly Sealed
	
	
	X

	

	Risk Phrases

Safety Phrases
	Workplace exposure Limits (WEL) 

	R 20 Harmful by inhalation.

R 36/37/38 Irritating to eyes, respiratory system and skin.

R 42/43 May cause sensitisation by inhalation and skin contact.

Contains isocyanates. See information supplied by the manufacturer
	9016-87-9 diphenylmethanediisocyanate, isomeres and homologues
Short-term value: 0.07 mg/m³

Long-term value: 0.02 mg/m³

	

	Frequency & Duration of Exposure

	Amount Used

Small (Millilitres)
 FORMCHECKBOX 

Medium Litres

 X
Large Cubic Metres
 FORMCHECKBOX 

	How many times per day

1 – 5

 X
5 – 10

 FORMCHECKBOX 

More than 10
 FORMCHECKBOX 

	Duration

1 – 5 Minutes

 FORMCHECKBOX 

6 – 30 Minutes
 FORMCHECKBOX 

31 – 60 Minutes
 X
1 Hour & Above
 FORMCHECKBOX 


	SUBSTANCE PROPERTIES (Tick all that apply)
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	Oxidising
	Explosive
	Flammable
Highly Flammable
	Toxic
	Harmful or Irritant
	Corrosive
	Carcinogenic
Mutagenic
	Dangerous for environment

	
	
	
	
	X
	
	
	


	GHS SUBSTANCE PROPERTIES
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	Oxidising
	Explosive
	(Extremely) Flammable
	Toxic
	Harmful
	Corrosive
	Human Health
	Dangerous for environment
	Gas under pressure

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	X
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 



	Control Measures

	General Precautions
	First Aid Measures

	Ensure good ventilation/exhaust in workplaces.

Avoid contact with skin and eyes.

Avoid inhalation of vapours and spray mist. Extinguish all open flames, remove sources of ignition, avoid

sparks. Do not smoke. Do not empty into drains.
Keep away from food, beverages and animal feed.

Observe the usual precautionary measures when handling chemicals.
RESPIRATORY PROTECTION

If the solvent concentration is above TLV-values, respiratory equipment admitted for this purpose must be

worn.
EYE PROTECTION
Tightly sealed safety glasses.

HAND PROTECTION

Impervious gloves.


	AFTER INHALATION

Supply fresh air. If required, provide artificial respiration. Keep patient warm. Consult doctor if symptoms persist.

AFTER SKIN CONTACT

Wash immediately with water and soap and rinse thoroughly.

Remove contaminated clothing.

AFTER EYE CONTACT
Rinse opened eye for several minutes under running water. Then consult doctor.

AFTER INGESTION
Do not induce vomiting; call for medical help immediately.

Rinse out mouth and then drink plenty of water.     

	
	

	Further Controls Required
	Responsibility
	By When
	Date Done

	N/A
	     
	     
	     

	

	Spillage Procedure
	Fire Prevention

	Keep people at a distance and stay on the windward side.
Do not allow to enter sewage system, surface or ground water.

Remove mechanically: Cover remains with damp, liquid-binding material (e.g. sawdust, chemical binders on a calcium silicate-hydrate base, sand). After approx. 1 hour, take up and place in refuse container. Do not close (CO2-development!) Keep damp and allow to stand in a safe place outdoors for several days.
	Extinguish all open flames, remove sources of ignition, avoid

sparks. Do not smoke.
CO2, extinguishing powder or water jet. Fight larger fires with water jet or alcohol-resistant foam.
Protective equipment: Wear self-contained breathing apparatus.

	Handling and Storage
	Disposal Considerations

	Ensure good ventilation/exhaust in workplaces.

Avoid contact with skin and eyes.

Avoid inhalation of vapours and spray mist. Extinguish all open flames, remove sources of ignition, avoid

sparks. Do not smoke. Do not empty into drains.
Store only in the original container.
Store between 15 and 30°C.
	Do not dispose of together with household garbage. Do not allow product to reach sewage system.
Must be specially treated in compliance with official regulations.
· European waste catalogue:

08 00 00 WASTES FROM THE MANUFACTURE, FORMULATION, SUPPLY AND USE (MFSU) OF COATINGS (PAINTS, VARNISHES AND VITREOUS ENAMELS), ADHESIVES, SEALANTS AND PRINTING INKS

08 05 00 wastes not otherwise specified in 08

08 05 01 waste isocyanates

	


	Assessor Summary
	
	YES/NO
	Further action

	1.
Has the assessment considered all factors 
pertinent to the use of the substance?  If NO 
please give 
details of further action required
	YES
	     

	2.
Has the assessment considered the 
practicability of preventing exposure?  If NO 
please give 
details of further action required
	YES
	     

	3.
Has the assessment considered the steps to 
be taken to achieve and maintain adequate 
control of exposure where prevention is not 
reasonably practicable?  If NO please give 
details of further action required
	YES
	     

	4.
Has the assessment considered the need for 
monitoring exposure to the substance  If NO 
please give details of further action required
	YES
	     

	5.
Has the assessment identified all action 
required to comply with regulations  If NO 
please give details of further action required
	YES
	     

	

	COSHH Assessment
	Please tick
	

	

	The task is safe to be carried out with current control procedures.
	X
	Tick if no further action required

	The task is safe to be carried out subject to actions listed
	     
	Tick if use of the substance is not causing significant problems but requires some action to bring it within COSHH guidelines, Action should be prioritised and specific dates set for completion

	Task/Substance is Unsafe, significant non-compliance with Health & Safety standards
	     
	Tick if the task or substance has potential to cause significant problems to users, use of substance to be discontinued until problems have been rectified
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