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	Name of Substance
	No Nonsense Line Marking Paint
	COSHH

Reference 
	C032     

	Supplied By
	No Nonsense Ltd
	Date of 
Assessment
	25/07/25

	Persons at Risk
	Staff
       X
	Public          FORMCHECKBOX 

	Young/Pregnant

Workers                FORMCHECKBOX 

	Review Date
	24/07/26

	
	Visitors       X 
	Contractor   X
	
	
	

	Description of Substance
	Marker Paint
	Method of use
	750ml Aerosol Spray

	

	Hazards Identification and PPE

	Routes of Entry
	Personal Protective Equipment (Tick Required Boxes)
	Tick here for none
 FORMCHECKBOX 


	Inhalation
X
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	Absorption
X
	
	
	
	
	
	
	

	Ingestion
X
	
	
	
	
	
	
	

	Location
	Hand Protection
	Protective clothing
	Protective Footwear
	Safety Glasses
	Face Shield
	Face Mask
	Respirator

	     
	X
	X
	X
	X
	
	
	

	

	Risk Phrases

Safety Phrases
	Workplace exposure Limits (WEL) 

	P210, P211, P251, P271, P305+P351+P338, P312, P410+P412, P501, P102
	N/A

	

	Frequency & Duration of Exposure

	Amount Used

Small (Millilitres)
X
Medium Litres

 
Large Cubic Metres
 FORMCHECKBOX 

	How many times per day

1 – 5

 X
5 – 10

 FORMCHECKBOX 

More than 10
 FORMCHECKBOX 

	Duration

1 – 5 Minutes

 FORMCHECKBOX 

6 – 30 Minutes
 FORMCHECKBOX 

31 – 60 Minutes
 FORMCHECKBOX 

1 Hour & Above
 X

	SUBSTANCE PROPERTIES (Tick all that apply)
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	Oxidising
	Explosive
	Flammable
Highly Flammable
	Toxic
	Harmful or Irritant
	Corrosive
	Carcinogenic
Mutagenic
	Dangerous for environment

	
	
	x
	
	x
	
	
	x


	GHS SUBSTANCE PROPERTIES
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	Oxidising
	Explosive
	(Extremely) Flammable
	Toxic
	Harmful
	Corrosive
	Human Health
	Dangerous for environment
	Gas under pressure

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 



	Control Measures

	General Precautions
	First Aid Measures

	Keep away from heat, sparks and open flame. Read and follow manufacturer's recommendations. Avoid inhalation of vapours and spray/mists. When sprayed on a naked flame or any incandescent material the aerosol vapours can be ignited. Avoid inhalation of vapours.

Appropriate engineering controls 

Provide adequate ventilation. 

Personal protection Wear protective work clothing. 

 Eye/face protection The following protection should be worn: Chemical splash goggles. Personal protective equipment for eye and face protection should comply with European Standard EN166. 

 Hand protection Chemical-resistant, impervious gloves complying with an approved standard should be worn if a risk assessment indicates skin contact is possible. Wear protective gloves made of the following material: Laminate >480 minutes. For users with sensitive skin, it is recommended that suitable protective gloves are worn. 

 Other skin and body protection 

 Provide eyewash station. Wear protective clothing. For the greatest protection, clothing should include anti-static overalls, boots and gloves. Wear anti-static protective clothing if there is a risk of ignition from static electricity. 

 Hygiene measures Wash promptly if skin becomes contaminated. Ensure the ventilation system is regularly maintained and tested. When using do not eat, drink or smoke. 

 Respiratory protection No specific recommendations. Respiratory protection must be used if the airborne contamination exceeds the recommended occupational exposure limit. If ventilation is inadequate, suitable respiratory protection must be worn. 

 Thermal hazards Spray will evaporate and cool rapidly and may cause frostbite or cold burns if in contact with skin. 


	Description of first aid measures:

· General information - Move affected person to fresh air at once. Get medical attention if any discomfort continues. Never give anything by mouth to an unconscious person. 

· Inhalation -  Move affected person to fresh air at once. If breathing stops, provide artificial respiration. Keep affected person warm and at rest. Get medical attention immediately. 
· Ingestion - Rinse mouth thoroughly with water. Do not induce vomiting. Get medical attention. 
· Skin contact - Wash skin thoroughly with soap and water. Get medical attention if any discomfort continues. 
· Eye contact - Rinse immediately with plenty of water. Continue to rinse for at least 15 minutes. Remove any contact lenses and open eyelids wide apart. Get medical attention immediately. Continue to rinse. 



	
	

	Further Controls Required
	Responsibility
	By When
	Date Done

	     N/A
	     
	     
	     

	

	Spillage Procedure
	Fire Prevention

	Environmental precautions - Avoid the spillage or runoff entering drains, sewers or watercourses. 

Methods for cleaning up - Eliminate all sources of ignition. No smoking, sparks, flames or other sources of ignition near spillage. Provide adequate ventilation. Wear suitable protective equipment, including gloves, goggles/face shield, respirator, boots, clothing or apron, as appropriate. Provide adequate ventilation. Contain spillage with sand, earth or other suitable non-combustible material. Avoid the spillage or runoff entering drains, sewers or watercourses. Absorb in vermiculite, dry sand or earth and place into containers.
	Keep away from heat, sparks and open flame. Read and follow manufacturer's recommendations. Avoid inhalation of vapours and spray/mists. When sprayed on a naked flame or any incandescent material the aerosol vapours can be ignited. Avoid inhalation of vapours.

	
	

	Handling and Storage
	Disposal Considerations

	· Storage precautions -  Store at moderate temperatures in dry, well ventilated area. Keep away from heat, sparks and open flame. Pressurised container: Must not be exposed to temperatures above 50°C. 
· Storage class Extremely - Flammable Aerosol 
· Transport info - This product is packed in accordance with the Limited quantity Provisions of CDGCPL2, ADR and IMDG. These provisions allow the transport of aerosols of less than 1 litre packed in cartons of less than 30kg gross weight to be exempt from control providing they are labelled in accordance with the requirements of those regulations to show that they are transported as Limited Quantities. Aerosols not so packed must show the following.


	General information Do not puncture or incinerate, even when empty. Ensure containers are empty before discarding (explosion risk). Dispose of waste to licensed waste disposal site in accordance with the requirements of the local Waste Disposal Authority. 

Disposal methods Containers should be thoroughly emptied before disposal because of the risk of an explosion. Do not puncture or incinerate, even when empty. Dispose of waste to licensed waste disposal site in accordance with the requirements of the local Waste Disposal Authority. Waste class Empty Aerosol: 15 01 10 (Containing hazardous residues). Full or Partially Empty Aerosol: 16 05 04, Empty Aerosol: 15 01 04 (No hazardous residues)

	


	COSHH Assessment Comments

	     


	Assessor Summary
	
	YES/NO
	Further action

	1.
Has the assessment considered all factors 
pertinent to the use of the substance?  If NO 
please give 
details of further action required
	YES
	     

	2.
Has the assessment considered the 
practicability of preventing exposure?  If NO 
please give 
details of further action required
	YES
	     

	3.
Has the assessment considered the steps to 
be taken to achieve and maintain adequate 
control of exposure where prevention is not 
reasonably practicable?  If NO please give 
details of further action required
	    YES 
	     

	4.
Has the assessment considered the need for 
monitoring exposure to the substance  If NO 
please give details of further action required
	YES  
	     

	5.
Has the assessment identified all action 
required to comply with regulations  If NO 
please give details of further action required
	YES   
	     

	

	COSHH Assessment
	Please tick
	

	

	The task is safe to be carried out with current control procedures.
	X
	Tick if no further action required

	The task is safe to be carried out subject to actions listed
	     
	Tick if use of the substance is not causing significant problems but requires some action to bring it within COSHH guidelines, Action should be prioritised and specific dates set for completion

	Task/Substance is Unsafe, significant non-compliance with Health & Safety standards
	     
	Tick if the task or substance has potential to cause significant problems to users, use of substance to be discontinued until problems have been rectified

	     
The Task/process should be re-assessed on a regular basis either annually, or if there are significant changes to the task or process or if there is a significant change in personnel who carry it out it e.g. young/inexperienced workers, pregnancy, workers with pre existing conditions such as asthma, dermatitis etc

Signed:  Assessor





Date     
……………………………………………………………………
………………………………………

This Assessment has been discussed with the user their line manager and action agreed

Signed:
User
     



Line Manager 
     


           Date     
……………………………………….
……………………………….……

……………..
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