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	Name of Substance
	No Nonsense Contact Adhesive
	COSHH

Reference 
	C050

	Supplied By
	No Nonsense
	Date of 
Assessment
	25/07/25

	Persons at Risk
	Staff
       X
	Public          X
	
	Review Date
	24/07/26

	
	Visitors       X
	Contractor   X
	
	
	

	Description of Substance
	Contact Adhesive
	Method of use
	Apply Directly on to intended surface

	

	Hazards Identification and PPE

	Routes of Entry
	Personal Protective Equipment (Tick Required Boxes)
	Tick here for none
 FORMCHECKBOX 


	Inhalation
X
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	Absorption
X
	
	
	
	
	
	
	

	Ingestion
X
	
	
	
	
	
	
	

	Location
	Hand Protection
	Protective clothing
	Protective Footwear
	Safety Glasses
	Face Shield
	Face Mask
	Respirator

	     
	X
	X
	
	X
	
	
	X

	

	Risk Phrases

Safety Phrases
	Workplace exposure Limits (WEL) 

	R51/53 Toxic to aquatic organisms, may cause long-term adverse effects in the aquatic environment.

R67 Vapours may cause drowsiness and dizziness.

S9 Keep container in a well-ventilated place.

S16 Keep away from sources of ignition - No smoking.

S24/25 Avoid contact with skin and eyes.

S26 In case of contact with eyes, rinse immediately with plenty of water and seek medical advice.

S29/56 Do not empty into drains, dispose of this material and its container at hazardous or special waste collection point.

S37 Wear suitable gloves.

S46 If swallowed, seek medical advice immediately and show this container or label.

S51 Use only in well-ventilated areas.

S61 Avoid release to the environment. Refer to special instructions/safety data sheets.

S64 If swallowed, rinse mouth with water (only if the person is conscious).
	ACETONE WEL 500 ppm 1210 mg/m3 1500 ppm 3620 mg/m3

CYCLOHEXANE WEL 100 ppm 350 mg/m3 300 ppm 1050 mg/m3

ETHYL ACETATE WEL 200 ppm 400 ppm

	

	Frequency & Duration of Exposure

	Amount Used

Small (Millilitres)
 X
Medium (Litres)
 FORMCHECKBOX 

Large (Cubic Metres)
 FORMCHECKBOX 

	How many times per day

1 – 5

 X
5 – 10

 FORMCHECKBOX 

More than 10
 FORMCHECKBOX 

	Duration

1 – 5 Minutes

 FORMCHECKBOX 

6 – 30 Minutes
 X
31 – 60 Minutes
 FORMCHECKBOX 
 
1 Hour & Above
 FORMCHECKBOX 



	SUBSTANCE PROPERTIES (Tick all that apply)
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	Oxidising
	Explosive
	Flammable
Highly Flammable
	Toxic
	Harmful or Irritant
	Corrosive
	Carcinogenic
Mutagenic
	Dangerous for environment

	
	
	X
	
	X
	
	
	X


	GHS SUBSTANCE PROPERTIES
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	Oxidising
	Explosive
	(Extremely) Flammable
	Toxic
	Harmful
	Corrosive
	Human Health
	Dangerous for environment
	Gas under pressure

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	X
	 FORMCHECKBOX 

	X
	 FORMCHECKBOX 

	X
	X
	 FORMCHECKBOX 



	Control Measures

	General Precautions
	First Aid Measures

	ENGINEERING MEASURES

Provide adequate ventilation. Observe Workplace Exposure Limits and minimise the risk of inhalation of vapours. Ensure that lighting and electrical equipment are not sources of ignition.

RESPIRATORY EQUIPMENT

If exposure limits are likely to be exceeded, use a full face mask fitted with an organic filter for short term exposures. For long term or high level exposures, or when spraying, compressed airline breathing apparatus should be used.

HAND PROTECTION

Protective gloves should be used if there is a risk of direct contact or splash. Use protective gloves made of: Viton rubber (fluor rubber).

EYE PROTECTION

Wear approved safety goggles.

SKIN PROTECTION

Wear apron or protective clothing in case of splashes.
	INHALATION

There may be irritation of the throat with a feeling of tightness in the chest. Exposure may cause coughing or wheezing. In case of persistent throat irritation or coughing: Seek medical attention and bring these instructions.

INGESTION

If conscious, give 1 pint of water to drink immediately. Rince mouth out with water, do not induce vomiting, provide fresh air and keep patient at rest. Seek medical attention.

SKIN CONTACT

There may be irritation and redness at the site of contact Promptly flush contaminated skin with soap or mild detergent and water. Promptly remove clothing if penetrated and flush the skin with water. Get medical attention if any discomfort continues.

EYE CONTACT

Immediately flush with plenty of water for up to 15 minutes. Remove any contact lenses and open eyelids widely. If irritation persists: Continue flushing during transport to hospital. Bring these instructions.

	
	

	Further Controls Required
	Responsibility
	By When
	Date Done

	N/A
	     
	     
	     

	

	Spillage Procedure
	Fire Prevention

	PERSONAL PRECAUTIONS

Refer to section 8 of SDS for personal protection details. Turn leaking containers leak-side up to prevent escape of liquid. Mark contaminated areas with signs and prevent access to unauthorised personnel.

ENVIRONMENTAL PRECAUTIONS

Avoid discharge into water courses or onto the ground.
SPILL CLEAN UP METHODS

Absorb in vermiculite, dry sand or earth and place into containers.
	EXTINGUISHING MEDIA

Use: Foam, carbon dioxide or dry powder. Cool containers with water spray.

SPECIFIC HAZARDS

The product is flammable, and heating may generate vapours which may form explosive vapour/air mixtures. In case of fire, toxic gases may be formed.

PROTECTIVE MEASURES IN FIRE

Self contained breathing apparatus and full protective clothing must be worn in case of fire.

	Handling and Storage
	Disposal Considerations

	USAGE PRECAUTIONS

Provide good ventilation. Avoid forming spray mists/aerosols. Keep away from heat, sparks and open flame. Static electricity and formation of sparks must be prevented.

STORAGE PRECAUTIONS

Keep away from heat, sparks and open flame. Keep containers tightly closed. Store in a cool place.
	Arrange disposal with a licensed waste disposal company.

	

	Assessor Summary
	
	YES/NO
	Further action

	1.
Has the assessment considered all factors 
pertinent to the use of the substance?  If NO 
please give 
details of further action required
	YES
	     

	2.
Has the assessment considered the 
practicability of preventing exposure?  If NO 
please give 
details of further action required
	YES
	     

	3.
Has the assessment considered the steps to 
be taken to achieve and maintain adequate 
control of exposure where prevention is not 
reasonably practicable?  If NO please give 
details of further action required
	YES
	     

	4.
Has the assessment considered the need for 
monitoring exposure to the substance  If NO 
please give details of further action required
	YES
	     

	5.
Has the assessment identified all action 
required to comply with regulations  If NO 
please give details of further action required
	YES
	     

	

	COSHH Assessment
	Please tick
	

	

	The task is safe to be carried out with current control procedures.
	X
	Tick if no further action required

	The task is safe to be carried out subject to actions listed
	     
	Tick if use of the substance is not causing significant problems but requires some action to bring it within COSHH guidelines, Action should be prioritised and specific dates set for completion

	Task/Substance is Unsafe, significant non-compliance with Health & Safety standards
	     
	Tick if the task or substance has potential to cause significant problems to users, use of substance to be discontinued until problems have been rectified
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