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	Name of Substance
	Gyproc Easi Fill 60
	COSHH

Reference 
	C054

	Supplied By
	British Gypsum
	Date of 
Assessment
	25/07/25

	Persons at Risk
	Staff
       X
	Public          X
	
	Review Date
	24/07/26

	
	Visitors       X
	Contractor   X
	
	
	

	Description of Substance
	Filler
	Method of use
	Mix with water and apply60 minute working time, with easy mixing, applying and sanding60 minute working time, with easy mixing, applying and sanding

	

	Hazards Identification and PPE

	Routes of Entry
	Personal Protective Equipment (Tick Required Boxes)
	Tick here for none
 FORMCHECKBOX 


	Inhalation
X
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	Absorption
X
	
	
	
	
	
	
	

	Ingestion
X
	
	
	
	
	
	
	

	Location
	Hand Protection
	Protective clothing
	Protective Footwear
	Safety Glasses
	Face Shield
	Face Mask
	Respirator

	     
	X
	X
	
	X
	
	
	X

	

	Risk Phrases

Safety Phrases
	Workplace exposure Limits (WEL) 

	Hazard Statements:

H302 - Harmful if swallowed

H332 - Harmful if inhaled

H335 - May cause respiratory irritation

Precautionary Statements: 
P261, P271, P304 + P340, P312,

P301 + P330, P305 + P313, P337 + P351, P264, P405, P403

+ P233, P270, P280, P285, P501
	Calcium Sulphate Hemihydrate - 10mg/m3 8hr TWA (Total Inhalable) - 4mg/m3 8hr TWA (Respirable)
Quartz (silica) - 0.1mg/m3 8hr TWA (Respirable)

	

	Frequency & Duration of Exposure

	Amount Used

Small (Millilitres)
 FORMCHECKBOX 

Medium (Litres)
 X
Large (Cubic Metres)
 FORMCHECKBOX 

	How many times per day

1 – 5

 X
5 – 10

 FORMCHECKBOX 

More than 10
 FORMCHECKBOX 

	Duration

1 – 5 Minutes

 FORMCHECKBOX 

6 – 30 Minutes
 FORMCHECKBOX 

31 – 60 Minutes
 X
1 Hour & Above
 FORMCHECKBOX 


	SUBSTANCE PROPERTIES (Tick all that apply)
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	Oxidising
	Explosive
	Flammable
Highly Flammable
	Toxic
	Harmful or Irritant
	Corrosive
	Carcinogenic
Mutagenic
	Dangerous for environment

	
	
	
	
	
	
	
	


	GHS SUBSTANCE PROPERTIES

	[image: image17.png]&




	[image: image18.png]



	[image: image19.png]



	[image: image20.png]



	[image: image21.png]



	[image: image22.png]



	[image: image23.png]



	[image: image24.png]



	[image: image25.png]




	Oxidising
	Explosive
	(Extremely) Flammable
	Toxic
	Harmful
	Corrosive
	Human Health
	Dangerous for environment
	Gas under pressure

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 



	Control Measures

	General Precautions
	First Aid Measures


General Get medical attention if any symptoms persist.
	     
	

	
	

	Further Controls Required
	Responsibility
	By When
	Date Done

	N/A
	     
	     
	     

	

	Spillage Procedure
	Fire Prevention

	Ensure adequate general ventilation of work areas to keep dust levels as low as possible. Do not eat, drink or smoke during use. Use personal protective equipment that is clean and has been properly maintained – store in a clean place away from the work area.
	The product does not pose a fire hazard. However, some packaging materials may burn. Suitable extinguishing media – water, foam, carbon dioxide or dry powder.

	Handling and Storage
	Disposal Considerations

	Manual handling – Supplied in up to 25kg bags – use an appropriate lifting technique.
Mechanical handling – To avoid potentially overloading a lift truck, it is important that any effect on load centres is considered. The nominal weight of each palletised load is given within the weights table in this section of this document.

Storage – Store in dry conditions. All powdered products can settle in transport. To maintain stability, place pallets on firm level ground, and ensure that stacks are both level and vertical.

Do not stack more than one lift high.

P403 + P233 - Store in a well ventilated place. Keep container

tightly closed

P405 - Store locked up.
	Waste treatment methods. Do not pour into drains or waterways. Wastes from gypsum products are normally classified as ‘non-hazardous’ but should not be co-disposed with municipal waste.

P501 - Dispose of contents of containers at an authorised landfill site in accordance with the Waste Management Licensing Regulations. (See Section 16 Other Information).

	

	Assessor Summary
	
	YES/NO
	Further action

	1.
Has the assessment considered all factors 
pertinent to the use of the substance?  If NO 
please give 
details of further action required
	YES
	     

	2.
Has the assessment considered the 
practicability of preventing exposure?  If NO 
please give 
details of further action required
	YES
	     

	3.
Has the assessment considered the steps to 
be taken to achieve and maintain adequate 
control of exposure where prevention is not 
reasonably practicable?  If NO please give 
details of further action required
	YES
	     

	4.
Has the assessment considered the need for 
monitoring exposure to the substance  If NO 
please give details of further action required
	YES
	     

	5.
Has the assessment identified all action 
required to comply with regulations  If NO 
please give details of further action required
	YES
	     

	

	COSHH Assessment
	Please tick
	

	

	The task is safe to be carried out with current control procedures.
	X
	Tick if no further action required

	The task is safe to be carried out subject to actions listed
	     
	Tick if use of the substance is not causing significant problems but requires some action to bring it within COSHH guidelines, Action should be prioritised and specific dates set for completion

	Task/Substance is Unsafe, significant non-compliance with Health & Safety standards
	     
	Tick if the task or substance has potential to cause significant problems to users, use of substance to be discontinued until problems have been rectified


[image: image26.png]