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	Name of Substance
	ARDEX X7R Grey Tile Adhesive
	COSHH

Reference 
	C003

	Supplied By
	Ardex UK Ltd
	Date of 
Assessment
	25/07/25

	Persons at Risk
	Staff
       X
	Public          FORMCHECKBOX 

	Young/Pregnant

Workers                FORMCHECKBOX 

	Review Date
	24/07/26

	
	Visitors       X
	Contractor   X
	
	
	

	Description of Substance
	Tile Adhesive
	Method of use
	For fixing ceramic, porcelain, glass mosaics, and most non-moisture sensitive natural stone floor and wall tiles. 


	

	Hazards Identification and PPE

	Routes of Entry
	Personal Protective Equipment (Tick Required Boxes)
	Tick here for none
 FORMCHECKBOX 


	Inhalation
X
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	Absorption
X
	
	
	
	
	
	
	

	Ingestion
X
	
	
	
	
	
	
	

	Location
	Hand Protection
	Protective clothing
	Protective Footwear
	Safety Glasses
	Face Shield
	Face Mask
	Respirator

	     
	X
	
	
	X
	
	X
Type P2 Dust protection
	

	

	Risk Phrases

Safety Phrases
	Occupational Exposure Standard (OES)
	Maximum Exposure Limits (MEL)
	Workplace exposure Limits (WEL) 

	Portland Cement
H315 - Causes skin irritation

H318 - Causes serious eye damage
	N/A
	N/A
	TWA – Portland

cement respirable dust; 4 mg/m 8 hrs 

	

	Frequency & Duration of Exposure

	Amount Used

Small (Millilitres)
 FORMCHECKBOX 

Medium Litres

 X
Large Cubic Metres
 FORMCHECKBOX 

	How many times per day

1 – 5

 X
5 – 10

 FORMCHECKBOX 

More than 10
 FORMCHECKBOX 

	Duration

1 – 5 Minutes

 FORMCHECKBOX 

6 – 30 Minutes
 FORMCHECKBOX 

31 – 60 Minutes
 FORMCHECKBOX 

1 Hour & Above
 X

	SUBSTANCE PROPERTIES (Tick all that apply)
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	Oxidising
	Explosive
	Flammable
Highly Flammable
	Toxic
	Harmful or Irritant
	Corrosive
	Carcinogenic
Mutagenic
	Dangerous for environment

	
	
	
	
	
	X
	
	


	GHS SUBSTANCE PROPERTIES
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	Oxidising
	Explosive
	(Extremely) Flammable
	Toxic
	Harmful
	Corrosive
	Human Health
	Dangerous for environment
	Gas under pressure

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	X
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 



	Control Measures

	General Precautions
	First Aid Measures

	Ensure good ventilation of the work station.
Respiratory protection not required in normal conditions. 
Dust formation: dust mask Type 2 or Type 3.
In case of splash hazard: safety glasses. 
Protective gloves to be worn, nitrile rubber recommended.
	Inhalation

Remove person to fresh air and keep comfortable for breathing.
Ingestion

If the person is fully conscious, make him/her drink plenty of water. Never give an unconscious person anything to drink.
Skin Contact

Wash skin with plenty of water. Take off contaminated clothing. If skin irritation occurs: Get medical advice/attention.
Eye Contact

Rinse cautiously with water for several minutes. Remove contact lenses, if present and easy to do. Continue rinsing. Call a physician immediately. 

	
	

	Further Controls Required
	Responsibility
	By When
	Date Done

	N/A
	     
	     
	     

	

	Spillage Procedure
	Fire Prevention

	Absorb spillage to prevent material damage.
Avoid contact with skin and eyes.
Prevent entry to sewers and public waters.
Recover mechanically the product. Minimize generation of dust. Collect spillage. Do not use

compressed air for cleaning.
	Product is non-combustible. Use fire extinguishing equipment appropriate for surrounding area.

	
	

	Handling and Storage
	Disposal Considerations

	Ensure good ventilation of the work station. Avoid contact with skin and eyes. Wear personal

protective equipment.

Wear protective gloves. Do not eat, drink or smoke when using this product.
Protect from moisture. Store in a dry place.
	Disposal must be done according to official regulations.

Dispose of contents/container in accordance with licensed collector’s sorting instructions.

Dispose in a safe manner in accordance with local/national regulations. Avoid release to the environment.



	


	COSHH Assessment Comments

	     

	


	Assessor Summary
	
	YES/NO
	Further action

	1.
Has the assessment considered all factors 
pertinent to the use of the substance?  If NO 
please give 
details of further action required
	YES
	     

	2.
Has the assessment considered the 
practicability of preventing exposure?  If NO 
please give 
details of further action required
	YES
	     

	3.
Has the assessment considered the steps to 
be taken to achieve and maintain adequate 
control of exposure where prevention is not 
reasonably practicable?  If NO please give 
details of further action required
	YES
	     

	4.
Has the assessment considered the need for 
monitoring exposure to the substance  If NO 
please give details of further action required
	YES
	     

	5.
Has the assessment identified all action 
required to comply with regulations  If NO 
please give details of further action required
	YES
	     

	

	COSHH Assessment
	Please tick
	

	

	The task is safe to be carried out with current control procedures.
	X
	Tick if no further action required

	The task is safe to be carried out subject to actions listed
	     
	Tick if use of the substance is not causing significant problems but requires some action to bring it within COSHH guidelines, Action should be prioritised and specific dates set for completion

	Task/Substance is Unsafe, significant non-compliance with Health & Safety standards
	     
	Tick if the task or substance has potential to cause significant problems to users, use of substance to be discontinued until problems have been rectified

	     
The Task/process should be re-assessed on a regular basis either annually, or if there are significant changes to the task or process or if there is a significant change in personnel who carry it out it e.g. young/inexperienced workers, pregnancy, workers with pre existing conditions such as asthma, dermatitis etc

Signed Assessor





Date     
……………………………………………………………………
………………………………………

This Assessment has been discussed with the user their line manager and action agreed

Signed:
User
     



Line Manager 
     


Date     
……………………………………….
……………………………….……

……………..
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