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	Name of Substance
	Construction Dust
	COSHH

Reference
	C008

	Supplied

By
	N/A
	Date of Assessment
	25/07/25

	Persons

at Risk
	Staff
	(
	Public
	(
	Young
	(
	Review

Date
	24/07/26

	
	Visitors
	(
	Contractors
	(
	Pregnant
	(
	
	

	Description of Substance
	Wood Dust, Silica Dust & Lower Toxicity Dusts
	Method

of Use
	Dusts produced on a general construction site


	Hazards Identification and PPE

	Routes of Entry
	Personal Protective Equipment Required (Tick as Appropriate)

	Inhalation
	(
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	Absorption
	(
	
	
	
	
	
	
	

	Ingestion
	(
	Hand Protection
	Protective Clothing
	Protective Footwear
	Safety Glasses
	Face

Shield
	Face

Mask
	Respirator

	Comments:
	
	
	
	
	
	(
	

	
	
	
	
	
	
	P3 Filter
	


	Risk Phrases

Safety Phrases
	Occupational

Exposure Standard

(OES)
	Maximum

Exposure Limits

(MEL)
	Workplace

Exposure Limits

(WEL)

	
	N/A
	N/A
	N/A


	Frequency & Duration Exposure

	Amount Used
	Home many times per day
	Duration

	Small (Millilitres)
	
	1-5
	(
	1-5 Minutes
	

	Medium (Litres)
	(
	5-10
	
	6-30 Minutes
	

	Large (Cubic Meters)
	
	More than 10
	
	31-60 Minutes
	

	
	1 Hour & Above
	(


	GHS Substance Properties
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	Oxidising
	Explosive
	(Extremely) Flammable
	Toxic
	Harmful
	Corrosive
	Human Health
	Dangerous for environment
	Gas under pressure

	
	
	
	
	
	
	(
	
	


	Control Measures

	General Precautions
	First Aid Measures

	Water suppression of dust clouds.

On tool extraction where possible.

Provide adequate ventilation, including appropriate local extraction, to ensure that the defined occupational exposure limit is not exceeded.

Wear face mask / respirator if there is dust formation. Dust filter P3.

limiting the number of people near the work;

· rotating those doing the task;

· enclosing the work to stop dust escaping. Use

sheeting or temporary screens;

· general mechanical ventilation to remove dusty air

from the work area (eg in enclosed spaces such as

indoors);

· selecting work clothes that do not keep hold of

the dust.
	Inhalation

Get medical attention if any discomfort continues.

Ingestion

Rinse mouth thoroughly. Get medical attention if any discomfort continues.

Skin Contact

Rinse with water. Contact physician if discomfort continues. Contact physician if irritation continues.

Eye Contact

Immediately flush with plenty of water.Remove any contact lenses and open eyes wide apart. Contact physician if irritation persists. Do not rub eye. 


	Further Controls Required
	Responsibility
	By When
	Completed

	N/A
	
	
	


	Spillage Procedure
	Fire Prevention

	Avoid generation and spreading of dust. Remove spillage with vacuum cleaner. If not possible, collect spillage with shovel, broom or the like.
	Use gently applied water (eg a spray or mist), not jets to extinguish fire, to minimise the disturbance of dust.


	Handling and Storage
	Disposal Considerations

	Avoid contact with skin and eyes. Avoid eating, drinking and smoking when using the product. Avoid inhalation of dust.

Store in a dry place.
	Dispose of waste and residues in accordance with local authority requirements. Powder to be collected, sealed tightly in bags and disposed on approved landfills.


	Assessor Summary
	YES / NO
	Further Action

	Has the assessment considered all factors pertinent to the use of the substance?

If NO please give details of further action required
	YES
	

	Has the assessment considered the practicability of preventing exposure?

If NO please give 
details of further action required
	YES
	

	Has the assessment considered the steps to 
be taken to achieve and maintain adequate control of exposure where prevention is not reasonably practicable?

If NO please give 
details of further action required
	YES
	

	Has the assessment considered the need for monitoring exposure to the substance?

If NO please give details of further action required
	YES
	

	Has the assessment identified all action required to comply with regulations?

If NO please give details of further action required
	YES
	


	COSHH Assessment

	The task is safe to be carried out with current control procedures.
	(
	No further action required

	The task is safe to be carried out subject to actions listed
	
	Use of the substance is not causing significant problems but requires some action to bring it within COSHH guidelines, Action should be prioritised and specific dates set for completion

	Task/Substance is Unsafe, significant non-compliance with Health & Safety standards
	
	Task or substance has potential to cause significant problems to users, use of substance to be discontinued until problems have been rectified
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