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	Name of Substance
	BAL MICROMAX 2
	COSHH

Reference 
	C009     

	Supplied By
	BAL – Building Adhesives Ltd
	Date of 
Assessment
	25/07/25

	Persons at Risk
	Staff
       X
	Public          FORMCHECKBOX 

	Young/Pregnant

Workers                FORMCHECKBOX 

	Review Date
	24/07/26

	
	Visitors       X 
	Contractor   X
	
	
	

	Description of Substance
	Cement based grout.
	Method of use
	Grouting ceramics and mosaics.

	

	Hazards Identification and PPE

	Routes of Entry
	Personal Protective Equipment (Tick Required Boxes)
	Tick here for none
 FORMCHECKBOX 


	Inhalation
X
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	Absorption
X
	
	
	
	
	
	
	

	Ingestion
X
	
	
	
	
	
	
	

	Location
	Hand Protection
	Protective clothing
	Protective Footwear
	Safety Glasses
	Face Shield
	Face Mask
	Respirator

	     
	X
	X
	
	X
	
	X
	

	

	Risk Phrases

Safety Phrases
	Occupational Exposure Standard (OES)
	Maximum Exposure Limits (MEL)
	Workplace exposure Limits (WEL) 

	P102 Keep out of reach of children.

P261 Avoid breathing dust.

P280 Wear protective gloves/ protective clothing/ eye protection/ face protection.

P305+P351+P338 IF IN EYES: Rinse cautiously with water for several minutes. Remove

contact lenses, if present and easy to do. Continue rinsing.

P501 Dispose of contents/ container in accordance with local regulations.
	N/A     
	N/A     
	N/A     

	

	Frequency & Duration of Exposure

	Amount Used

Small (Millilitres)
 FORMCHECKBOX 

Medium Litres

 X
Large Cubic Metres
 FORMCHECKBOX 

	How many times per day

1 – 5

 X
5 – 10

 FORMCHECKBOX 

More than 10
 FORMCHECKBOX 

	Duration

1 – 5 Minutes

 FORMCHECKBOX 

6 – 30 Minutes
 FORMCHECKBOX 

31 – 60 Minutes
 FORMCHECKBOX 

1 Hour & Above
 X

	SUBSTANCE PROPERTIES (Tick all that apply)
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	Oxidising
	Explosive
	Flammable
Highly Flammable
	Toxic
	Harmful or Irritant
	Corrosive
	Carcinogenic
Mutagenic
	Dangerous for environment

	
	
	
	
	
	
	
	


	GHS SUBSTANCE PROPERTIES
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	Oxidising
	Explosive
	(Extremely) Flammable
	Toxic
	Harmful
	Corrosive
	Human Health
	Dangerous for environment
	Gas under pressure

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 



	Control Measures

	General Precautions
	First Aid Measures

	Provide adequate ventilation. Avoid inhalation of dust. 
The following protection should be worn: Chemical splash goggles.
Chemical-resistant, impervious gloves complying with an approved standard should be worn if

a risk assessment indicates skin contact is possible.
Do not smoke in work area. Wash at the end of each work shift and before eating, smoking and using the toilet. Wash promptly if skin becomes contaminated. Promptly remove any clothing that becomes contaminated. When using do not eat, drink or smoke.
Protection against nuisance dust must be used when the airborne concentration exceeds 10 mg/m3. (P3 Filter Protection to be Worn).
	Inhalation
Move exposed person to fresh air at once. Rinse nose and mouth with water. Get medical attention if any discomfort continues.
Ingestion
Rinse mouth thoroughly with water. Get medical attention if any discomfort continues.
Skin Contact 
Remove affected person from source of contamination. Remove contaminated clothing. Wash skin thoroughly with soap and water. Get medical attention if any discomfort continues.
Eye contact 
Remove any contact lenses and open eyelids wide apart. Continue to rinse for at least 15 minutes. Continue to rinse for at least 15 minutes. Get medical attention if any discomfort

continues.

	
	


	Further Controls Required
	Responsibility
	By When
	Date Done

	N/A
	     
	     
	     

	

	Spillage Procedure
	Fire Prevention

	Avoid generation and spreading of dust. 
Collect and place in suitable waste disposal containers and seal securely. Label the containers containing waste and contaminated materials and remove from the area as soon as possible. 
Flush contaminated area with plenty of water.
	Product is non flammable. Use fire extinguishing equipment appropriate for surrounding area.

	
	

	Handling and Storage
	Disposal Considerations

	Avoid spilling. Avoid contact with skin and eyes. Avoid handling which leads to dust formation.
Store in tightly closed original container in a dry, cool and well-ventilated place.
	Dispose of waste to licensed waste disposal site in accordance with the requirements of the local Waste Disposal Authority.

	


	COSHH Assessment Comments

	     


	Assessor Summary
	
	YES/NO
	Further action

	1.
Has the assessment considered all factors 
pertinent to the use of the substance?  If NO 
please give 
details of further action required
	YES
	     

	2.
Has the assessment considered the 
practicability of preventing exposure?  If NO 
please give 
details of further action required
	YES
	     

	3.
Has the assessment considered the steps to 
be taken to achieve and maintain adequate 
control of exposure where prevention is not 
reasonably practicable?  If NO please give 
details of further action required
	    YES 
	     

	4.
Has the assessment considered the need for 
monitoring exposure to the substance  If NO 
please give details of further action required
	YES  
	     

	5.
Has the assessment identified all action 
required to comply with regulations  If NO 
please give details of further action required
	YES   
	     

	

	COSHH Assessment
	Please tick
	

	

	The task is safe to be carried out with current control procedures.
	X
	Tick if no further action required

	The task is safe to be carried out subject to actions listed
	     
	Tick if use of the substance is not causing significant problems but requires some action to bring it within COSHH guidelines, Action should be prioritised and specific dates set for completion

	Task/Substance is Unsafe, significant non-compliance with Health & Safety standards
	     
	Tick if the task or substance has potential to cause significant problems to users, use of substance to be discontinued until problems have been rectified

	     
The Task/process should be re-assessed on a regular basis either annually, or if there are significant changes to the task or process or if there is a significant change in personnel who carry it out it e.g. young/inexperienced workers, pregnancy, workers with pre existing conditions such as asthma, dermatitis etc

Signed:  Assessor





Date     
……………………………………………………………………
………………………………………

This Assessment has been discussed with the user their line manager and action agreed

Signed:
User
     



Line Manager 
     


           Date     
……………………………………….
……………………………….……

……………..
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