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	Name of Substance
	Satinwood
	COSHH

Reference 
	C018     

	Supplied By
	Dulux Trade
	Date of 
Assessment
	25/07/25

	Persons at Risk
	Staff
       X
	Public          FORMCHECKBOX 

	Young/Pregnant

Workers                FORMCHECKBOX 

	Review Date
	24/07/26

	
	Visitors       X 
	Contractor   X
	
	
	

	Description of Substance
	Solvent based satin coating for wood/metal.
	Method of use
	Solvent borne coating for interior use.

	

	Hazards Identification and PPE

	Routes of Entry
	Personal Protective Equipment (Tick Required Boxes)
	Tick here for none
 FORMCHECKBOX 


	Inhalation
X
	[image: image1.jpg]



	[image: image2.jpg]



	[image: image3.jpg]



	[image: image4.jpg]



	[image: image5.jpg]



	[image: image6.jpg]



	[image: image7.jpg]




	Absorption
X
	
	
	
	
	
	
	

	Ingestion
X
	
	
	
	
	
	
	

	Location
	Hand Protection
	Protective clothing
	Protective Footwear
	Safety Glasses
	Face Shield
	Face Mask
	Respirator

	     
	X
	X
	
	X
	
	
	X

	

	Risk Phrases

Safety Phrases
	Workplace exposure Limits (WEL) 

	H226 – Flammable Liquid & Vapour

P102, P101, P210, P233, P262, P312, P235, P501
2-ethylhexanoic acid, zirconium salt
	N/A     
TWA: 5 mg/m³ - 8Hours

STEL:10 mg/m³ - 15 minutes

	

	Frequency & Duration of Exposure

	Amount Used

Small (Millilitres)
 FORMCHECKBOX 

Medium Litres

 X
Large Cubic Metres
 FORMCHECKBOX 

	How many times per day

1 – 5

 X
5 – 10

 FORMCHECKBOX 

More than 10
 FORMCHECKBOX 

	Duration

1 – 5 Minutes

 FORMCHECKBOX 

6 – 30 Minutes
 FORMCHECKBOX 

31 – 60 Minutes
 FORMCHECKBOX 

1 Hour & Above
 X

	SUBSTANCE PROPERTIES (Tick all that apply)
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	Oxidising
	Explosive
	Flammable
Highly Flammable
	Toxic
	Harmful or Irritant
	Corrosive
	Carcinogenic
Mutagenic
	Dangerous for environment

	
	
	X
	
	X
	
	
	


	GHS SUBSTANCE PROPERTIES
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	Oxidising
	Explosive
	(Extremely) Flammable
	Toxic
	Harmful
	Corrosive
	Human Health
	Dangerous for environment
	Gas under pressure

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	X
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 



	Control Measures

	General Precautions
	First Aid Measures


position and seek medical advice.

	Inhalation – Remove to fresh air. Keep person warm and at rest. If not breathing, if breathing is irregular or if respiratory arrest occurs, provide artificial respiration or oxygen by

trained personnel.

Ingestion – If swallowed, seek medical advice immediately and show the container or label. Keep person warm and at rest. Do NOT induce vomiting

Skin contact – Remove contaminated clothing and shoes. Wash skin thoroughly with soap and water or use recognised skin cleanser. Do NOT use solvents or thinners.

Eye contact –Remove contact lenses, irrigate copiously with clean, fresh water, holding the eyelids apart for at least 10 minutes and seek immediate medical advice.     
	

	
	

	Further Controls Required
	Responsibility
	By When
	Date Done

	     N/A
	     
	     
	     

	

	Spillage Procedure
	Fire Prevention

	Contain and collect spillage with non-combustible, absorbent material e.g. sand, earth, vermiculite or diatomaceous earth and place in container for disposal according to local regulations. Preferably clean with a detergent. Avoid using solvents.
	Information on fire and explosion protection Vapours are heavier than air and may spread along floors. Vapours may form explosive mixtures with air.
Recommended: alcohol-resistant foam, CO₂, powders, water spray. Do not use water jet.
Fire will produce dense black smoke. Exposure to decomposition products may cause a health hazard. Cool closed containers exposed to fire with water. Do not release runoff from fire to drains or watercourses.

	
	

	Handling and Storage
	Disposal Considerations

	Prevent the creation of flammable or explosive concentrations of vapours in air and avoid vapour concentrations higher than the occupational exposure limits.

In addition, the product should only be used in areas from which all naked lights and other sources of ignition have been excluded. Electrical equipment should be protected to the appropriate standard.

Mixture may charge electrostatically: always use earthing leads when transferring from one container to another.
Operators should wear antistatic footwear and clothing and floors should be of the conducting type.

Keep away from heat, sparks and flame. No sparking tools should be used.
Avoid contact with skin and eyes. Avoid the inhalation of dust, particulates, spray or mist arising from the application of this mixture. Avoid inhalation of dust from sanding.

Eating, drinking and smoking should be prohibited in areas where this material is handled, stored and processed.

Put on appropriate personal protective equipment.

Never use pressure to empty. Container is not a pressure vessel. Always keep in containers made from the same material as the original one.
Comply with the health and safety at work laws.

Do not allow to enter drains or watercourses.

.
	Do not allow to enter drains or watercourses.
Dispose of according to all federal, state and local applicable regulations.
If this product is mixed with other wastes, the original waste product code may no longer apply and the appropriate code should be assigned. 

The generation of waste should be avoided or minimised wherever possible.
Disposal of this product, solutions and any by-products should at all times comply with the requirements of environmental protection and waste disposal legislation and any regional local authority requirements. 
Dispose of surplus and nonrecyclable

products via a licensed waste disposal contractor. 
Waste should not be disposed of untreated to the sewer unless fully compliant with the requirements of all authorities with jurisdiction.


	


	COSHH Assessment Comments

	     


	Assessor Summary
	
	YES/NO
	Further action

	1.
Has the assessment considered all factors 
pertinent to the use of the substance?  If NO 
please give 
details of further action required
	YES
	     

	2.
Has the assessment considered the 
practicability of preventing exposure?  If NO 
please give 
details of further action required
	YES
	     

	3.
Has the assessment considered the steps to 
be taken to achieve and maintain adequate 
control of exposure where prevention is not 
reasonably practicable?  If NO please give 
details of further action required
	    YES 
	     

	4.
Has the assessment considered the need for 
monitoring exposure to the substance  If NO 
please give details of further action required
	YES  
	     

	5.
Has the assessment identified all action 
required to comply with regulations  If NO 
please give details of further action required
	YES   
	     

	

	COSHH Assessment
	Please tick
	

	

	The task is safe to be carried out with current control procedures.
	X
	Tick if no further action required

	The task is safe to be carried out subject to actions listed
	     
	Tick if use of the substance is not causing significant problems but requires some action to bring it within COSHH guidelines, Action should be prioritised and specific dates set for completion

	Task/Substance is Unsafe, significant non-compliance with Health & Safety standards
	     
	Tick if the task or substance has potential to cause significant problems to users, use of substance to be discontinued until problems have been rectified

	     
The Task/process should be re-assessed on a regular basis either annually, or if there are significant changes to the task or process or if there is a significant change in personnel who carry it out it e.g. young/inexperienced workers, pregnancy, workers with pre existing conditions such as asthma, dermatitis etc

Signed:  Assessor





Date     
……………………………………………………………………
………………………………………

This Assessment has been discussed with the user their line manager and action agreed

Signed:
User
     



Line Manager 
     


           Date     
……………………………………….
……………………………….……

……………..
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