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	Name of Substance
	ALTRO CRETE SLIP RESISTANT AGGREGATE
	COSHH

Reference 
	C025

	Supplied By
	Altro Resin Systems Ltd
	Date of 
Assessment
	25/07/25

	Persons at Risk
	Staff
       X
	Public          X
	Young/Pregnant

Workers                FORMCHECKBOX 

	Review Date
	24/07/26

	
	Visitors       X
	Contractor   X
	
	
	

	Description of Substance
	Aggregate/Filler for Resin Screed/Self-Leveller
	Method of use
	Used in conjunction with Altro Crete Polyeurathane Flooring System

	

	Hazards Identification and PPE

	Routes of Entry
	Personal Protective Equipment (Tick Required Boxes)
	Tick here for none
 FORMCHECKBOX 


	Inhalation
X
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	Absorption
X
	
	
	
	
	
	
	

	Ingestion
X
	
	
	
	
	
	
	

	Location
	Hand Protection
	Protective clothing
	Protective Footwear
	Safety Glasses
	Face Shield
	Face Mask
	Respirator

	     
	X
	X
	
	X
	
	
	X

	

	Risk Phrases

Safety Phrases
	Workplace exposure Limits (WEL) 

	H315 Causes skin irritation.

H318 Causes serious eye damage.

H334 May cause allergy or asthma symptoms or breathing difficulties if inhaled.      
	No specific assessment has been carried out for the mixture

	

	Frequency & Duration of Exposure

	Amount Used

Small (Millilitres)
 FORMCHECKBOX 

Medium Litres

 X
Large Cubic Metres
 FORMCHECKBOX 

	How many times per day

1 – 5

 X
5 – 10

 FORMCHECKBOX 

More than 10
 FORMCHECKBOX 

	Duration

1 – 5 Minutes

 FORMCHECKBOX 

6 – 30 Minutes
 FORMCHECKBOX 

31 – 60 Minutes
 FORMCHECKBOX 

1 Hour & Above
 X

	SUBSTANCE PROPERTIES (Tick all that apply)
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	Oxidising
	Explosive
	Flammable
Highly Flammable
	Toxic
	Harmful or Irritant
	Corrosive
	Carcinogenic
Mutagenic
	Dangerous for environment

	
	
	X
	
	X
	
	
	


	GHS SUBSTANCE PROPERTIES
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	Oxidising
	Explosive
	(Extremely) Flammable
	Toxic
	Harmful
	Corrosive
	Human Health
	Dangerous for environment
	Gas under pressure

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	X
	X
	 FORMCHECKBOX 

	 FORMCHECKBOX 



	Control Measures

	General Precautions
	First Aid Measures

	Do not eat, drink or smoke in work areas. Wash hands after use. Remove contaminated clothing and protective equipment before entering eating areas.
RESPIRATORY PROTECTION

Avoid airborne dust generation. Provide appropriate exhaust ventilation at places where airborne dust is generated. In case of insufficient ventilation, wear suitable protective equipment. Handle packaged products carefully to prevent accidental bursting. 
EYE PROTECTION
Wear safety glasses with side-shields in circumstances where there is a risk of penetrative eye injuries.

HAND PROTECTION

Appropriate protection (e.g. protective clothing, barrier cream) is recommended for workers

who suffer from dermatitis or sensitive skin. Wash hands at the end of each work session.

ENVIRONMENTAL EXPOSURE CONTROLS
Avoid wind dispersal.
	AFTER INHALATION

Remove casualty from exposure ensuring one’s own safety whilst doing so. Seek medical attention if you feel unwell.

AFTER SKIN CONTACT

Wash immediately with plenty of soap and water.


AFTER EYE CONTACT
Flush with plenty of water. Seek medical attention if irritation persists.

AFTER INGESTION
Wash out mouth with water. Do not induce vomiting. Seek medical attention if you feel unwell.     

	
	

	Further Controls Required
	Responsibility
	By When
	Date Done

	N/A
	     
	     
	     

	

	Spillage Procedure
	Fire Prevention

	Avoid dry sweeping and use water spraying or vacuum cleaning systems to prevent airborne

dust generation. Wear personal protective equipment in compliance with national legislation.
	No specific extinguishing media is needed.
Non-combustible. No hazardous thermal decomposition.

No specific fire-fighting protection is required.

	Handling and Storage
	Disposal Considerations

	Minimise airborne dust generation and prevent wind dispersal during the loading and unloading. Keep containers closed and store packaged products so as to prevent bursting.
Do not eat, drink or smoke in work areas. Wash hands after use. Remove contaminated

clothing and protective equipment before entering eating areas.
	Recycling and disposal of packaging should be carried out in compliance with local regulations.

The re-use of packaging is not recommended. Recycling and disposal of packaging should be carried out by an authorised waste management company.

Where possible, recycling is preferred to disposal. Can be disposed of in compliance with local regulations.

	


	Assessor Summary
	
	YES/NO
	Further action

	1.
Has the assessment considered all factors 
pertinent to the use of the substance?  If NO 
please give 
details of further action required
	YES
	     

	2.
Has the assessment considered the 
practicability of preventing exposure?  If NO 
please give 
details of further action required
	YES
	     

	3.
Has the assessment considered the steps to 
be taken to achieve and maintain adequate 
control of exposure where prevention is not 
reasonably practicable?  If NO please give 
details of further action required
	YES
	     

	4.
Has the assessment considered the need for 
monitoring exposure to the substance  If NO 
please give details of further action required
	YES
	     

	5.
Has the assessment identified all action 
required to comply with regulations  If NO 
please give details of further action required
	YES
	     

	

	COSHH Assessment
	Please tick
	

	

	The task is safe to be carried out with current control procedures.
	X
	Tick if no further action required

	The task is safe to be carried out subject to actions listed
	     
	Tick if use of the substance is not causing significant problems but requires some action to bring it within COSHH guidelines, Action should be prioritised and specific dates set for completion

	Task/Substance is Unsafe, significant non-compliance with Health & Safety standards
	     
	Tick if the task or substance has potential to cause significant problems to users, use of substance to be discontinued until problems have been rectified
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