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	Name of Substance
	Remmers Crete RT (Resin Component)
	COSHH

Reference 
	C029

	Supplied By
	Remmers Baustofftechnik GmbH
	Date of 
Assessment
	25/07/25

	Persons at Risk
	Staff
       X
	Public          X
	Young/Pregnant

Workers                FORMCHECKBOX 

	Review Date
	24/07/26

	
	Visitors       X
	Contractor   X
	
	
	

	Description of Substance
	Resin Component part of a 3-component polyurethane screed system.
	Method of use
	Water dispersed polyurethane resin system combined with graded silica aggregates.

	

	Hazards Identification and PPE

	Routes of Entry
	Personal Protective Equipment (Tick Required Boxes)
	Tick here for none
 FORMCHECKBOX 


	Inhalation
X
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	Absorption
X
	
	
	
	
	
	
	

	Ingestion
X
	
	
	
	
	
	
	

	Location
	Hand Protection
	Protective clothing
	Protective Footwear
	Safety Glasses
	Face Shield
	Face Mask
	Respirator

	     
	X
	X
	
	X
Tightly Sealed
	
	
	

	

	Risk Phrases

Safety Phrases
	Workplace exposure Limits (WEL) 

	When used and handled according to directions, the product does not have any harmful effects according to the information available.
	No exposure limit value known for the mixture     

	

	Frequency & Duration of Exposure

	Amount Used

Small (Millilitres)
 FORMCHECKBOX 

Medium Litres

 X
Large Cubic Metres
 FORMCHECKBOX 

	How many times per day

1 – 5

 X
5 – 10

 FORMCHECKBOX 

More than 10
 FORMCHECKBOX 

	Duration

1 – 5 Minutes

 FORMCHECKBOX 

6 – 30 Minutes
 FORMCHECKBOX 

31 – 60 Minutes
 FORMCHECKBOX 

1 Hour & Above
 X

	SUBSTANCE PROPERTIES (Tick all that apply)
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	Oxidising
	Explosive
	Flammable
Highly Flammable
	Toxic
	Harmful or Irritant
	Corrosive
	Carcinogenic
Mutagenic
	Dangerous for environment

	
	
	
	
	
	
	
	


	GHS SUBSTANCE PROPERTIES
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	Oxidising
	Explosive
	(Extremely) Flammable
	Toxic
	Harmful
	Corrosive
	Human Health
	Dangerous for environment
	Gas under pressure

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 



	Control Measures

	General Precautions
	First Aid Measures

	Do not eat, drink or smoke in work areas. Wash hands after use. Remove contaminated clothing and protective equipment before entering eating areas.
RESPIRATORY PROTECTION

Under normal handling conditions respiratory protection not required.
EYE PROTECTION
Tightly sealed safety glasses.

HAND PROTECTION

Impervious gloves.


	AFTER INHALATION

Supply fresh air. If required, provide artificial respiration. Keep patient warm. Consult doctor if symptoms persist.

AFTER SKIN CONTACT

Wash immediately with water and soap and rinse thoroughly.

Remove contaminated clothing.

AFTER EYE CONTACT
Rinse opened eye for several minutes under running water. Then consult doctor.

AFTER INGESTION
Do not induce vomiting; call for medical help immediately.

Rinse out mouth and then drink plenty of water.     

	
	

	Further Controls Required
	Responsibility
	By When
	Date Done

	N/A
	     
	     
	     

	

	Spillage Procedure
	Fire Prevention

	Keep people at a distance and stay on the windward side.
Do not allow to enter sewage system, surface or ground water.
Absorb with liquid-binding material (sand, diatomite, acid binders, universal binders, sawdust).
No dangerous materials are released.
	CO2, extinguishing powder or water jet. Fight larger fires with water jet or alcohol-resistant foam.
Protective equipment: Wear self-contained breathing apparatus.

	Handling and Storage
	Disposal Considerations

	No special measures required for safe handling.
Store only in the original container.
Do not store above +30 °C.

Avoid cooling down to below 10°C.
	Do not dispose of together with household garbage. Do not allow product to reach sewage system.
Must be specially treated in compliance with official regulations.

	


	Assessor Summary
	
	YES/NO
	Further action

	1.
Has the assessment considered all factors 
pertinent to the use of the substance?  If NO 
please give 
details of further action required
	YES
	     

	2.
Has the assessment considered the 
practicability of preventing exposure?  If NO 
please give 
details of further action required
	YES
	     

	3.
Has the assessment considered the steps to 
be taken to achieve and maintain adequate 
control of exposure where prevention is not 
reasonably practicable?  If NO please give 
details of further action required
	YES
	     

	4.
Has the assessment considered the need for 
monitoring exposure to the substance  If NO 
please give details of further action required
	YES
	     

	5.
Has the assessment identified all action 
required to comply with regulations  If NO 
please give details of further action required
	YES
	     

	

	COSHH Assessment
	Please tick
	

	

	The task is safe to be carried out with current control procedures.
	X
	Tick if no further action required

	The task is safe to be carried out subject to actions listed
	     
	Tick if use of the substance is not causing significant problems but requires some action to bring it within COSHH guidelines, Action should be prioritised and specific dates set for completion

	Task/Substance is Unsafe, significant non-compliance with Health & Safety standards
	     
	Tick if the task or substance has potential to cause significant problems to users, use of substance to be discontinued until problems have been rectified
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