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	Name of Substance
	Remmers Crete RT (Aggregate Component)
	COSHH

Reference 
	C031

	Supplied By
	Remmers Baustofftechnik GmbH
	Date of 
Assessment
	25/07/25

	Persons at Risk
	Staff
       X
	Public          X
	Young/Pregnant

Workers                FORMCHECKBOX 

	Review Date
	24/07/26

	
	Visitors       X
	Contractor   X
	
	
	

	Description of Substance
	Aggregate Component part of a 3-component polyurethane screed system.
	Method of use
	Water dispersed polyurethane resin system combined with graded silica aggregates.

	

	Hazards Identification and PPE

	Routes of Entry
	Personal Protective Equipment (Tick Required Boxes)
	Tick here for none
 FORMCHECKBOX 


	Inhalation
X
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	Absorption
X
	
	
	
	
	
	
	

	Ingestion
X
	
	
	
	
	
	
	

	Location
	Hand Protection
	Protective clothing
	Protective Footwear
	Safety Glasses
	Face Shield
	Face Mask
	Respirator

	     
	X
	X
	
	X
Tightly Sealed
	
	
	X
P2 Filter

	

	Risk Phrases

Safety Phrases
	Workplace exposure Limits (WEL) 

	Dangerous Components: Cement
R 41 Risk of serious damage to eyes.
R36/38 Irritating to eyes and skin.

R43 May cause sensitisation by skin contact.
S22 Do not breathe dust.

S26 In case of contact with eyes, rinse immediately with plenty of water and seek medical advice.

S39 Wear eye/face protection.
	Long-term value: 10* 4** mg/m³

*inhalable dust **respirable dust

	

	Frequency & Duration of Exposure

	Amount Used

Small (Millilitres)
 FORMCHECKBOX 

Medium Litres

 X
Large Cubic Metres
 FORMCHECKBOX 

	How many times per day

1 – 5

 X
5 – 10

 FORMCHECKBOX 

More than 10
 FORMCHECKBOX 

	Duration

1 – 5 Minutes

 FORMCHECKBOX 

6 – 30 Minutes
 FORMCHECKBOX 

31 – 60 Minutes
 X
1 Hour & Above
 FORMCHECKBOX 


	SUBSTANCE PROPERTIES (Tick all that apply)
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	Oxidising
	Explosive
	Flammable
Highly Flammable
	Toxic
	Harmful or Irritant
	Corrosive
	Carcinogenic
Mutagenic
	Dangerous for environment

	
	
	
	
	X
	
	
	


	GHS SUBSTANCE PROPERTIES
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	Oxidising
	Explosive
	(Extremely) Flammable
	Toxic
	Harmful
	Corrosive
	Human Health
	Dangerous for environment
	Gas under pressure

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	X
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 



	Control Measures

	General Precautions
	First Aid Measures

	Immediately remove soiled, saturated clothing.

Do not eat, drink or smoke while working.

Keep away from food, beverages and animal feed.

Use skin protection cream for preventive skin protection.

Wash hands before pauses and after work.

Avoid contact with eyes and skin.

Do not inhale dust / smoke / mist.

Observe Professional Association regulations.
Avoid the formation of dust.

Protect against moisture.

Keep out of reach of children.

Avoid skin contact.

Avoid eye contact.
RESPIRATORY PROTECTION

Short term filter device:

Filter P2.
EYE PROTECTION
Tightly sealed safety glasses.
BODY PROTECTION
Protective Work Clothing.

HAND PROTECTION

Impervious gloves.


	AFTER INHALATION

Seek medical treatment in case of complaints.

AFTER SKIN CONTACT

Wash immediately with water and soap and rinse thoroughly.

Remove contaminated clothing.
If skin irritation continues, consult a doctor.

AFTER EYE CONTACT
Rinse opened eye for several minutes under running water. Then consult doctor.
AFTER INGESTION
Do not induce vomiting; call for medical help immediately.

Rinse out mouth and then drink plenty of water.     

	
	

	Further Controls Required
	Responsibility
	By When
	Date Done

	N/A
	     
	     
	     

	

	Spillage Procedure
	Fire Prevention

	Avoid uncontrolled admittance of water.

Avoid uncontrolled runoff after admittance of water.

Avoid runoff into sewage system and receiving water.
Collect mechanically.

Keep away from water.
	Use fire fighting measures that suit the environment.
No special measures required.

	Handling and Storage
	Disposal Considerations

	Avoid the formation of dust.

Protect against moisture.

Keep out of reach of children.

Avoid skin contact.

Avoid eye contact.
Store in closed rooms protected against moisture.

Extraction of dust in compliance with BImSchG or Technical Instructions Air. Keep container tightly closed.

Store dry.
	Disposal must be made according to official regulations

Hardens after contact with water. After hardening it can be disposed of as concrete (European waste catalogue: EWC-Code: 170101).

	


	Assessor Summary
	
	YES/NO
	Further action

	1.
Has the assessment considered all factors 
pertinent to the use of the substance?  If NO 
please give 
details of further action required
	YES
	     

	2.
Has the assessment considered the 
practicability of preventing exposure?  If NO 
please give 
details of further action required
	YES
	     

	3.
Has the assessment considered the steps to 
be taken to achieve and maintain adequate 
control of exposure where prevention is not 
reasonably practicable?  If NO please give 
details of further action required
	YES
	     

	4.
Has the assessment considered the need for 
monitoring exposure to the substance  If NO 
please give details of further action required
	YES
	     

	5.
Has the assessment identified all action 
required to comply with regulations  If NO 
please give details of further action required
	YES
	     

	

	COSHH Assessment
	Please tick
	

	

	The task is safe to be carried out with current control procedures.
	X
	Tick if no further action required

	The task is safe to be carried out subject to actions listed
	     
	Tick if use of the substance is not causing significant problems but requires some action to bring it within COSHH guidelines, Action should be prioritised and specific dates set for completion

	Task/Substance is Unsafe, significant non-compliance with Health & Safety standards
	     
	Tick if the task or substance has potential to cause significant problems to users, use of substance to be discontinued until problems have been rectified
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