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	Name of Substance
	SikaScreed® HardTop-60
	COSHH

Reference 
	C033     

	Supplied By
	Sika
	Date of 
Assessment
	25/07/25

	Persons at Risk
	Staff
       X
	Public          FORMCHECKBOX 

	Young/Pregnant

Workers                FORMCHECKBOX 

	Review Date
	24/07/26

	
	Visitors       X 
	Contractor   X
	
	
	

	Description of Substance
	Levelling Mortar
	Method of use
	Work the freshly mixed system into the concrete substrate with a stiff brush or level with a squeegee and roll it afterwards.

	

	Hazards Identification and PPE

	Routes of Entry
	Personal Protective Equipment (Tick Required Boxes)
	Tick here for none
 FORMCHECKBOX 


	Inhalation
X
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	Absorption
X
	
	
	
	
	
	
	

	Ingestion
X
	
	
	
	
	
	
	

	Location
	Hand Protection
	Protective clothing
	Protective Footwear
	Safety Glasses
	Face Shield
	Face Mask
	Respirator

	     
	X
	X
	
	X
	
	x
	

	

	Risk Phrases

Safety Phrases
	Workplace exposure Limits (WEL) 

	P101, P102, P103, P280, P305, P351, P338, P310
	N/A

	

	Frequency & Duration of Exposure

	Amount Used

Small (Millilitres)
X
Medium Litres

 
Large Cubic Metres
 FORMCHECKBOX 

	How many times per day

1 – 5

 X
5 – 10

 FORMCHECKBOX 

More than 10
 FORMCHECKBOX 

	Duration

1 – 5 Minutes

 FORMCHECKBOX 

6 – 30 Minutes
 FORMCHECKBOX 

31 – 60 Minutes
 FORMCHECKBOX 

1 Hour & Above
 X

	SUBSTANCE PROPERTIES (Tick all that apply)
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	Oxidising
	Explosive
	Flammable
Highly Flammable
	Toxic
	Harmful or Irritant
	Corrosive
	Carcinogenic
Mutagenic
	Dangerous for environment

	
	
	
	
	
	x
	
	


	GHS SUBSTANCE PROPERTIES
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	Oxidising
	Explosive
	(Extremely) Flammable
	Toxic
	Harmful
	Corrosive
	Human Health
	Dangerous for environment
	Gas under pressure

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	x
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 



	Control Measures

	General Precautions
	First Aid Measures

	Personal precautions :  Use personal protective equipment. Avoid breathing dust. Deny access to unprotected persons.
Personal protective equipment 

Eye protection :  Safety glasses with side-shields conforming to EN166 Eye wash bottle with pure water 

Hand protection : Chemical-resistant, impervious gloves complying with an approved standard must be worn at all times when handling chemical products. Reference number EN 374. Follow manufacturer specifications. 

Recommended: Butyl rubber/nitrile rubber gloves. Contaminated gloves should be removed. 

Skin and body protection :  Dust impervious protective suit Protective clothing (e.g. Safety shoes acc. to EN ISO 20345, long-sleeved working clothing, long trousers). Rubber aprons and protective boots are additionaly recommended for mixing and stirring work. 

Respiratory protection :  Respirator selection must be based on known or anticipated exposure levels, the hazards of the product and the safe working limits of the selected respirator. particulate filter P
	Description of first aid measures 

General advice :  Move out of dangerous area. Consult a physician. Show this safety data sheet to the doctor in attendance.
If inhaled :  Move to fresh air. Consult a physician after significant exposure. 

In case of skin contact :  Take off contaminated clothing and shoes immediately. Wash off with soap and plenty of water. If symptoms persist, call a physician. 

In case of eye contact :  Small amounts splashed into eyes can cause irreversible tissue damage and blindness. In the case of contact with eyes, rinse immediately with plenty of water and seek medical advice. Continue rinsing eyes during transport to hospital. Remove contact lenses. Keep eye wide open while rinsing. 

If swallowed :  Do not induce vomiting without medical advice. Rinse mouth with water. Do not give milk or alcoholic beverages. Never give anything by mouth to an unconscious person.
Most important symptoms and effects, both acute and delayed 

Symptoms : Excessive lachrymation See Section 11 for more detailed information on health effects and symptoms. 

Risks : No known significant effects or hazards. 

   Causes serious eye damage. 

Indication of any immediate medical attention and special treatment needed 

Treatment : Treat symptomatically.

	
	

	Further Controls Required
	Responsibility
	By When
	Date Done

	     N/A
	     
	     
	     

	

	Spillage Procedure
	Fire Prevention

	Methods for cleaning up :  Pick up and arrange disposal without creating dust. Keep in suitable, closed containers for disposal.
Environmental exposure controls 

General advice :  Try to prevent the material from entering drains or water courses. 


	Firefighting measures 

Extinguishing media 

Suitable extinguishing media :  Use extinguishing measures that are appropriate to local circumstances and the surrounding environment. 

Special hazards arising from the substance or mixture 

Hazardous combustion products 

No hazardous combustion products are known 

Advice for firefighters 

Special protective equipment for firefighters 

In the event of fire, wear self-contained breathing apparatus.  

Further information :  Standard procedure for chemical fires.  



	
	

	Handling and Storage
	Disposal Considerations

	 Precautions for safe handling 

Advice on safe handling :  Avoid exceeding the given occupational exposure limits (see section 8). Do not get in eyes, on skin, or on clothing. For personal protection see section 8. Smoking, eating and drinking should be prohibited in the application area. Follow standard hygiene measures when handling chemical products  

Advice on protection against fire and explosion 

:  Avoid dust formation. Provide appropriate exhaust ventilation at places where dust is formed.  

Hygiene measures :  Handle in accordance with good industrial hygiene and safety practice. When using do not eat or drink. When using do not smoke. Wash hands before breaks and at the end of workday.  

Conditions for safe storage, including any incompatibilities 

Requirements for storage areas and containers 

:  Keep container tightly closed in a dry and well-ventilated place. Store in accordance with local regulations.  

Other data : Keep in a dry place. No decomposition if stored and applied as directed.
	Waste treatment methods 

Product :  The generation of waste should be avoided or minimized wherever possible. Empty containers or liners may retain some product residues. This material and its container must be disposed of in a safe way. Dispose of surplus and non-recyclable products via a licensed waste disposal contractor. Disposal of this product, solutions and any by-products should at all times comply with the requirements of environmental protection and waste disposal legislation and any regional local authority requirements. Avoid dispersal of spilled material and runoff and contact with soil, waterways, drains and sewers. 

European Waste Catalogue :  17 09 04 mixed construction and demolition wastes other than those mentioned in 17 09 01, 17 09 02 and 17 09 03 

Contaminated packaging :  15 01 10* packaging containing residues of or contaminated by dangerous substances

	


	COSHH Assessment Comments

	     


	Assessor Summary
	
	YES/NO
	Further action

	1.
Has the assessment considered all factors 
pertinent to the use of the substance?  If NO 
please give 
details of further action required
	YES
	     

	2.
Has the assessment considered the 
practicability of preventing exposure?  If NO 
please give 
details of further action required
	YES
	     

	3.
Has the assessment considered the steps to 
be taken to achieve and maintain adequate 
control of exposure where prevention is not 
reasonably practicable?  If NO please give 
details of further action required
	    YES 
	     

	4.
Has the assessment considered the need for 
monitoring exposure to the substance  If NO 
please give details of further action required
	YES  
	     

	5.
Has the assessment identified all action 
required to comply with regulations  If NO 
please give details of further action required
	YES   
	     

	

	COSHH Assessment
	Please tick
	

	

	The task is safe to be carried out with current control procedures.
	X
	Tick if no further action required

	The task is safe to be carried out subject to actions listed
	     
	Tick if use of the substance is not causing significant problems but requires some action to bring it within COSHH guidelines, Action should be prioritised and specific dates set for completion

	Task/Substance is Unsafe, significant non-compliance with Health & Safety standards
	     
	Tick if the task or substance has potential to cause significant problems to users, use of substance to be discontinued until problems have been rectified

	     
The Task/process should be re-assessed on a regular basis either annually, or if there are significant changes to the task or process or if there is a significant change in personnel who carry it out it e.g. young/inexperienced workers, pregnancy, workers with pre existing conditions such as asthma, dermatitis etc

Signed:  Assessor





Date     
……………………………………………………………………
………………………………………

This Assessment has been discussed with the user their line manager and action agreed

Signed:
User
     



Line Manager 
     


           Date     
……………………………………….
……………………………….……

……………..
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