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	Name of Substance
	Stone and Marble Adhesive -MS76 Knifegrade
	COSHH

Reference 
	C039

	Supplied By
	Akemi
	Date of 
Assessment
	25/07/25

	Persons at Risk
	Staff
       X
	Public          X
	
	Review Date
	24/07/26

	
	Visitors       X
	Contractor   X
	
	
	

	Description of Substance
	Polyester Resin Adhesive
	Method of use
	Used for bonding natural and artificial stone to one another and to metal, wood and various plastics. 

	

	Hazards Identification and PPE

	Routes of Entry
	Personal Protective Equipment (Tick Required Boxes)
	Tick here for none
 FORMCHECKBOX 


	Inhalation
X
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	Absorption
X
	
	
	
	
	
	
	

	Ingestion
X
	
	
	
	
	
	
	

	Location
	Hand Protection
	Protective clothing
	Protective Footwear
	Safety Glasses
	Face Shield
	Face Mask
	Respirator

	     
	X
Nitrile
	X
	
	X
Tightly Sealed
	
	
	X
P2

	

	Risk Phrases

Safety Phrases
	Workplace exposure Limits (WEL) 

	Hazard Phrases:
H226 Flammable liquid and vapour
H304 May be Fatal if Swallowed and Enters Airways
H315 Causes skin irritation

H319 Causes serious eye irritation

H332 Harmful if inhaled

H335 May Cause respiratory irritation

H361d Suspected of damaging the unborn child

H372 Causes damage to the hearing organs through prolonged of repeated exposure

H400 Very toxic to aquatic life

H410 Very toxic to aquatic life with long lasting effects.

H412 Harmful to aquatic life with long lasting effects.
	Short Term Value: 1080mg/m³ 250ppm
Long Term Value: 430mg/m³ 100ppm

	

	Frequency & Duration of Exposure

	Amount Used

Small (Millilitres)
 FORMCHECKBOX 

Medium (Litres)
 X
Large (Cubic Metres)
 FORMCHECKBOX 

	How many times per day

1 – 5

 X
5 – 10

 FORMCHECKBOX 

More than 10
 FORMCHECKBOX 

	Duration

1 – 5 Minutes

 FORMCHECKBOX 

6 – 30 Minutes
 X
31 – 60 Minutes
 FORMCHECKBOX 
 
1 Hour & Above
 FORMCHECKBOX 


	SUBSTANCE PROPERTIES (Tick all that apply)
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	Oxidising
	Explosive
	Flammable
Highly Flammable
	Toxic
	Harmful or Irritant
	Corrosive
	Carcinogenic
Mutagenic
	Dangerous for environment

	
	
	X
	
	X
	
	
	X


	GHS SUBSTANCE PROPERTIES
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	Oxidising
	Explosive
	(Extremely) Flammable
	Toxic
	Harmful
	Corrosive
	Human Health
	Dangerous for environment
	Gas under pressure

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	X
	 FORMCHECKBOX 

	X
	 FORMCHECKBOX 

	X
	 FORMCHECKBOX 

	 FORMCHECKBOX 



	Control Measures

	General Precautions
	First Aid Measures

	Apply solvent resistant skin cream prior to works.

Do not eat, drink, smoke or sniff during works.

Keep away from foodstuffs.

Immediately remove soiled and contaminated clothing.

Wash hands before breaks and at the end of work.

Avoid contact with eyes and skin.

Use only in well ventilated areas and ensure good ventilation especially at floor level (fumes are heavier than air). 
RESPIRATORY PROTECTION

Filter A/P2
EYE PROTECTION
Tightly sealed safety goggles.

HAND PROTECTION

Nitrile Gloves
BODY PROTECTION

Protective Work Clothing

	AFTER INHALATION

Supply fresh air. If required provide artificial respiration. Keep patient warm. Consult doctor if symptoms persist.

AFTER SKIN CONTACT

Immediately wash with water and soap and rinse thoroughly. If skin irritation continues consult a doctor. 

AFTER EYE CONTACT
Rinse opened eye for several minutes under running water. If symptoms persist, consult a doctor.

AFTER INGESTION
If symptoms persist consult a doctor.     

	
	

	Further Controls Required
	Responsibility
	By When
	Date Done

	N/A
	     
	     
	     

	

	Spillage Procedure
	Fire Prevention

	Keep people at a distance. Wear protective equipment. Keep away from ignition sources. Use respiratory protective device against the effects of fumes/dust/aerosol. Ensure adequate ventilation. 
Do not allow to enter sewage system, surface or ground water. 
Absorb with liquid binding material (sand, diatomite, acid binders, universal binders, sawdust)
	Protect from Heat. Extinguish all open flames, remove sources of ignition, avoid sparks. Do not smoke.
Protect Against electrostatic charges.

Fumes can combine with air to form an explosive mixture.


	Handling and Storage
	Disposal Considerations

	Keep receptacles tightly sealed.

Store in a cool, dry place.

Keep away from heat and direct sunlight.
	Do not dispose of together with household garbage. Do not allow product to reach sewage system.
Must be specially treated in compliance with official regulations.


	


	Assessor Summary
	
	YES/NO
	Further action

	1.
Has the assessment considered all factors 
pertinent to the use of the substance?  If NO 
please give 
details of further action required
	YES
	     

	2.
Has the assessment considered the 
practicability of preventing exposure?  If NO 
please give 
details of further action required
	YES
	     

	3.
Has the assessment considered the steps to 
be taken to achieve and maintain adequate 
control of exposure where prevention is not 
reasonably practicable?  If NO please give 
details of further action required
	YES
	     

	4.
Has the assessment considered the need for 
monitoring exposure to the substance  If NO 
please give details of further action required
	YES
	     

	5.
Has the assessment identified all action 
required to comply with regulations  If NO 
please give details of further action required
	YES
	     

	

	COSHH Assessment
	Please tick
	

	

	The task is safe to be carried out with current control procedures.
	X
	Tick if no further action required

	The task is safe to be carried out subject to actions listed
	     
	Tick if use of the substance is not causing significant problems but requires some action to bring it within COSHH guidelines, Action should be prioritised and specific dates set for completion

	Task/Substance is Unsafe, significant non-compliance with Health & Safety standards
	     
	Tick if the task or substance has potential to cause significant problems to users, use of substance to be discontinued until problems have been rectified
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