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	Name of Substance
	SDHEX001 EGGER 04 Joint and Joist Adhesive

	COSHH

Reference 
	C043

	Supplied By
	   EGGER
	Date of 
Assessment
	25/07/25

	Persons at Risk
	Staff
       X
	Public          X
	
	Review Date
	24/07/26

	
	Visitors       X
	Contractor   X
	
	
	

	Description of Substance
	D4 grade adhesive conforming to

 EN204/D4
	Method of use
	Adhesive for the tongue & groove of the boards and applied to the joists.  

	

	Hazards Identification and PPE

	Routes of Entry
	Personal Protective Equipment (Tick Required Boxes)
	Tick here for none
 FORMCHECKBOX 


	Inhalation
X
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	Absorption
X
	
	
	
	
	
	
	

	Ingestion
X
	
	
	
	
	
	
	

	Location
	Hand Protection
	Protective clothing
	Protective Footwear
	Safety Glasses
	Face Shield
	Face Mask
	Respirator

	     
	
	
	
	
	
	
	

	

	Risk Phrases

Safety Phrases
	Workplace exposure Limits (WEL) 

	P201- Obtain special instructions before use.

P260- Do not breathe dust/fume/gas/mist/vapours/spray.

P280 – Wear protective gloves/ protective clothing/ eye protection/ face protection.
P284 – Wear respiratory protection.
P304 + P340 + P312  IF INHALED: Remove person to fresh air and keep comfortable for breathing. Call a Poison Centre or doctor/physician if you feel unwell.
P362 + P364 Take off contaminated clothing and wash it before re-use. 
	

	

	Frequency & Duration of Exposure

	Amount Used

Small (Millilitres)
 FORMCHECKBOX 

Medium (Litres)
 X
Large (Cubic Metres)
 FORMCHECKBOX 

	How many times per day

1 – 5

 X
5 – 10

 FORMCHECKBOX 

More than 10
 FORMCHECKBOX 

	Duration

1 – 5 Minutes

 FORMCHECKBOX 

6 – 30 Minutes
 FORMCHECKBOX 

31 – 60 Minutes
 FORMCHECKBOX 
 
1 Hour & Above
X

	SUBSTANCE PROPERTIES (Tick all that apply)
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	Oxidising
	Explosive
	Flammable
Highly Flammable
	Toxic
	Harmful or Irritant
	Corrosive
	Carcinogenic
Mutagenic
	Dangerous for environment

	
	
	
	
	
	
	
	


	GHS SUBSTANCE PROPERTIES
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	Oxidising
	Explosive
	(Extremely) Flammable
	Toxic
	Harmful
	Corrosive
	Human Health
	Dangerous for environment
	Gas under pressure

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	 FORMCHECKBOX 

	
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 



	Control Measures

	General Precautions
	First Aid Measures

	Ensure there is sufficient ventilation of the area.

Respiratory Protection: In case of insufficient ventilation wear suitable respiratory equipment. If exposure levels are likely to be exceeded use a face mask fitted with AXP3 filter for short-term low-level exposures, or for long term/high level exposures a positive pressure air fed mask should be used.
Hand Protection: Rubber Gloves 

Eye Protection: Safety Goggles 

Skin Protection: Protective work clothing to avoid skin contact.

OEL: Isocyanates all (as NCO) – MEL 8-hour TWA 0.02 mg/m3, STEL 15-minute 0.07 mg m/3 – Sen.

	General advice: If potential for exposure exists refer to Section 8 for specific personal protective equipment. First Aid responders should pay attention to self-protection and use the recommended protective clothing (chemical resistant gloves, splash protection).
Inhalation: Move person to fresh air. If not breathing, give artificial respiration; if by mouth-to-mouth use rescuer protection (pocket mask, etc). If breathing is difficult, oxygen should be administered by qualified personnel. Call a physician or transport to a medical facility.
Skin contact: Remove material from skin immediately by washing with soap and plenty of water. Remove contaminated clothing and shoes while washing. Seek medical attention if irritation persists. Wash clothing before reuse. An MDI skin decontamination study demonstrated that cleaning very soon after exposure is important, and that a polyglycol-based skin cleanser or corn oil may be more effective than soap and water. Discard items which cannot be decontaminated, including leather articles such as shoes, belts and watchbands. Suitable emergency safety shower facility should be available in work area.
Eye contact: Immediately flush eyes with water; remove contact lenses after the first 5 minutes, if present, then continue flushing eyes for at least 15 minutes. Obtain medical attention without delay, preferably from an ophthalmologist. Suitable emergency eye wash facility should be immediately available.
Ingestion: If swallowed, seek medical attention. Do not induce vomiting unless directed to do so by medical personnel.
     

	
	

	Further Controls Required
	Responsibility
	By When
	Date Done

	
	     
	     
	     

	

	Spillage Procedure
	Fire Prevention

	Contain spilled material if possible. Absorb with materials such as: Dirt. Vermiculite. Sand. Clay. Do NOT use absorbent materials such as: Cement powder (Note: may generate heat). Collect in suitable and properly labelled open containers. Do not place in sealed containers. Suitable containers include: Metal drums. Plastic drums.Polylined fibre packs. Wash the spill site with large quantities of water. Attempt to neutralize by adding suitable decontaminant solution: Formulation 1: sodium carbonate 5 -10%; liquid  detergent 0.2-  2%; water to make up to 100%, OR Formulation  2: concentrated ammonia solution 3- 8%; liquid detergent 0.2-  2%; water to make up to 100%. If ammonia is used, use good ventilation to prevent vapour exposure. Contact your supplier  for clean-up assistance.
	Suitable extinguishing media: Water fog or fine spray. Dry chemical fire extinguishers. Carbon dioxide fire extinguishers. Foam. Alcohol resistant foams (ATC type) are preferred. General purpose synthetic foams (including AFFF) or protein foams may function, but will be less effective.
Unsuitable extinguishing media: Do not use direct water stream. May spread fire.


	Handling and Storage
	Disposal Considerations

	Store in a cool, ventilated area. Keep container tightly closed.
Handling: Ensure there is sufficient ventilation of area. Avoid direct contact with the substance.  
	Licensed waste contractor to dispose of any waste product or its packaging. It is however the users responsibility to ensure wastes are disposed of in accordance with all valid laws.  

	


	Assessor Summary
	
	YES/NO
	Further action

	1.
Has the assessment considered all factors 
pertinent to the use of the substance?  If NO 
please give 
details of further action required
	YES
	     

	2.
Has the assessment considered the 
practicability of preventing exposure?  If NO 
please give 
details of further action required
	YES
	     

	3.
Has the assessment considered the steps to 
be taken to achieve and maintain adequate 
control of exposure where prevention is not 
reasonably practicable?  If NO please give 
details of further action required
	YES
	     

	4.
Has the assessment considered the need for 
monitoring exposure to the substance  If NO 
please give details of further action required
	YES
	     

	5.
Has the assessment identified all action 
required to comply with regulations  If NO 
please give details of further action required
	YES
	     

	

	COSHH Assessment
	Please tick
	

	

	The task is safe to be carried out with current control procedures.
	X
	Tick if no further action required

	The task is safe to be carried out subject to actions listed
	     
	Tick if use of the substance is not causing significant problems but requires some action to bring it within COSHH guidelines, Action should be prioritised and specific dates set for completion

	Task/Substance is Unsafe, significant non-compliance with Health & Safety standards
	     
	Tick if the task or substance has potential to cause significant problems to users, use of substance to be discontinued until problems have been rectified
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