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	Name of Substance
	Fire Pro Acoustic Intumescent Sealant 
	COSHH

Reference 
	C044

	Supplied By
	ROCKWOOL 
	Date of 
Assessment
	25/07/25

	Persons at Risk
	Staff
       X
	Public          X
	
	Review Date
	24/07/26

	
	Visitors       X
	Contractor   X
	
	
	

	Description of Substance
	ACOUSTIC INTUMESCENT SEALANT
	Method of use
	Sealing linear joints and

some individual service penetrations

passing through various substrates

	

	Hazards Identification and PPE

	Routes of Entry
	Personal Protective Equipment (Tick Required Boxes)
	Tick here for none
 FORMCHECKBOX 


	Inhalation
X
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	Absorption
X
	
	
	
	
	
	
	

	Ingestion
X
	
	
	
	
	
	
	

	Location
	Hand Protection
	Protective clothing
	Protective Footwear
	Safety Glasses
	Face Shield
	Face Mask
	Respirator

	     
	x
	x
	x
	x
	x
	x
	x

	

	Risk Phrases

Safety Phrases
	Workplace exposure Limits (WEL) 

	S2: Keep out of reach of children. 

S36/37/39: Wear suitable protective clothing, gloves and eye/face protection.
R22: Harmful if swallowed. 

R34: Causes burns. 

R36: Irritating to eyes.

R41: Risk of serious damage to eyes. 

R43: May cause sensitisation by skin contact.
R50: Very toxic to aquatic animals.

EUH208: Contains nuosept kmb. May produce an allergic reaction.
	

	

	Frequency & Duration of Exposure

	Amount Used

Small (Millilitres)
 FORMCHECKBOX 

Medium (Litres)
 X
Large (Cubic Metres)
 FORMCHECKBOX 

	How many times per day

1 – 5

 X
5 – 10

 FORMCHECKBOX 

More than 10
 FORMCHECKBOX 

	Duration

1 – 5 Minutes

 FORMCHECKBOX 

6 – 30 Minutes
 FORMCHECKBOX 

31 – 60 Minutes
 FORMCHECKBOX 
 
1 Hour & Above          X

	SUBSTANCE PROPERTIES (Tick all that apply)
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	Oxidising
	Explosive
	Flammable
Highly Flammable
	Toxic
	Harmful or Irritant
	Corrosive
	Carcinogenic
Mutagenic
	Dangerous for environment

	
	
	
	
	
	
	
	


	GHS SUBSTANCE PROPERTIES
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	Oxidising
	Explosive
	(Extremely) Flammable
	Toxic
	Harmful
	Corrosive
	Human Health
	Dangerous for environment
	Gas under pressure

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	 FORMCHECKBOX 

	
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 



	Control Measures

	General Precautions
	First Aid Measures


	Skin contact: Wash immediately with plenty of soap and water. Eye contact: Bathe the eye with running water for 15 minutes. Ingestion: Wash out mouth with water. Inhalation: Consult a doctor. 4.2 Most important symptoms and effects, both acute and delayed Skin contact: There may be mild irritation at the site of contact. Eye contact: There may be irritation and redness. Ingestion: There may be irritation of the throat. Inhalation: There may be irritation of the throat with a feeling of tightness in the chest.
     
	

	
	

	Further Controls Required
	Responsibility
	By When
	Date Done

	
	     
	     
	     

	

	Spillage Procedure
	Fire Prevention

	Personal precautions

Mark out the contaminated area with signs and prevent access to unauthorised personnel. 

6.2 Environmental precautions Environmental precautions: Do not discharge into drains or rivers.

6.3 Methods and material for containment and cleaning up Clean-up procedures: Transfer to a closable, labelled salvage container for disposal by an appropriate method.
	Extinguishing media: Suitable extinguishing media for the surrounding fire should be used. 
Suitable extinguishing media Water, foam, carbon dioxide or dry powder.

5.2 Special hazards arising from the substance or mixture Exposure hazards: In combustion emits toxic fumes. 

5.3 Advice for firefighters Advice for firefighters: Wear self-contained breathing apparatus. Wear protective clothing to prevent contact with skin and eyes.



	Handling and Storage
	Disposal Considerations

	Keep container tightly closed in a cool, dry and ventilated area.
	Disposal operations: Transfer to a suitable container and arrange for collection by specialised disposal company.

Disposal of packaging: 

Dispose of as normal industrial waste. 

NB: The user’s attention is drawn to the possible existence of regional or national regulations regarding disposal.

	


	Assessor Summary
	
	YES/NO
	Further action

	1.
Has the assessment considered all factors 
pertinent to the use of the substance?  If NO 
please give 
details of further action required
	YES
	     

	2.
Has the assessment considered the 
practicability of preventing exposure?  If NO 
please give 
details of further action required
	YES
	     

	3.
Has the assessment considered the steps to 
be taken to achieve and maintain adequate 
control of exposure where prevention is not 
reasonably practicable?  If NO please give 
details of further action required
	YES
	     

	4.
Has the assessment considered the need for 
monitoring exposure to the substance If NO 
please give details of further action required
	YES
	     

	5.
Has the assessment identified all action 
required to comply with regulations If NO 
please give details of further action required
	YES
	     

	

	COSHH Assessment
	Please tick
	

	

	The task is safe to be carried out with current control procedures.
	X
	Tick if no further action required

	The task is safe to be carried out subject to actions listed
	     
	Tick if use of the substance is not causing significant problems but requires some action to bring it within COSHH guidelines, Action should be prioritised and specific dates set for completion

	Task/Substance is Unsafe, significant non-compliance with Health & Safety standards
	     
	Tick if the task or substance has potential to cause significant problems to users, use of substance to be discontinued until problems have been rectified
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