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	Name of Substance
	MIRROR PRO
	COSHH

Reference 
	C048

	Supplied By
	SEAL IT SERVICES LTD
	Date of 
Assessment
	25/07/25

	Persons at Risk
	Staff
       X
	Public          X
	
	Review Date
	24/07/26

	
	Visitors       X
	Contractor   X
	
	
	

	Description of Substance
	Sealant/Adhesive.
	Method of use
	Apply directly to the intended surface.

	

	Hazards Identification and PPE

	Routes of Entry
	Personal Protective Equipment (Tick Required Boxes)
	Tick here for none
 FORMCHECKBOX 


	Inhalation
X
	[image: image1.jpg]



	[image: image2.jpg]



	[image: image3.jpg]



	[image: image4.jpg]



	[image: image5.jpg]



	[image: image6.jpg]



	[image: image7.jpg]




	Absorption
X
	
	
	
	
	
	
	

	Ingestion
X
	
	
	
	
	
	
	

	Location
	Hand Protection
	Protective clothing
	Protective Footwear
	Safety Glasses
	Face Shield
	Face Mask
	Respirator

	     
	
	X
	
	X
	
	
	

	

	Risk Phrases

Safety Phrases
	Workplace exposure Limits (WEL) 

	14 - 14.6. Special precautions for user.

14 - 14.7. Transport in bulk according to Annex II of MARPOL 73/78 and the IBC Code.

15 - 15.2. Chemical safety assessment.
Flam. Liq. 3: H226 - Flammable liquid and vapour.

Acute Tox. 4: H332 - Harmful if inhaled.

Skin Sens. 1: H317 - May cause an allergic skin reaction.

Eye Dam. 1: H318 - Causes serious eye damage.

Aquatic Chronic 2: H411 - Toxic to aquatic life with long lasting effects.
	No Information.

	

	Frequency & Duration of Exposure

	Amount Used

Small (Millilitres)
 X
Medium (Litres)
 FORMCHECKBOX 

Large (Cubic Metres)
 FORMCHECKBOX 

	How many times per day

1 – 5

 X
5 – 10

 FORMCHECKBOX 

More than 10
 FORMCHECKBOX 

	Duration

1 – 5 Minutes

 FORMCHECKBOX 

6 – 30 Minutes
 X
31 – 60 Minutes
 FORMCHECKBOX 
 
1 Hour & Above
 FORMCHECKBOX 


	SUBSTANCE PROPERTIES (Tick all that apply)
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	Oxidising
	Explosive
	Flammable
Highly Flammable
	Toxic
	Harmful or Irritant
	Corrosive
	Carcinogenic
Mutagenic
	Dangerous for environment

	
	
	
	
	X
	
	
	X


	GHS SUBSTANCE PROPERTIES
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	Oxidising
	Explosive
	(Extremely) Flammable
	Toxic
	Harmful
	Corrosive
	Human Health
	Dangerous for environment
	Gas under pressure

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	X
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	X
	 FORMCHECKBOX 



	Control Measures

	General Precautions
	First Aid Measures


	- Inhalation: Move the exposed person to fresh air.

- Eye contact: Rinse immediately with plenty of water for 15 minutes holding the eyelids open.

- Skin contact: Wash off immediately with plenty of soap and water. Remove contaminated clothing.

- Ingestion: DO NOT INDUCE VOMITING.
     
	

	
	

	Further Controls Required
	Responsibility
	By When
	Date Done

	N/A
	     
	     
	     

	

	Spillage Procedure
	Fire Prevention

	- Personal precautions, protective equipment and emergency procedures: Ensure adequate ventilation of the working area.

- Environmental precautions:  Do not allow product to enter drains. Prevent further spillage if safe.

- Methods and material for containment and cleaning up:  Absorb with inert, absorbent material. Sweep up. Transfer to suitable, labelled containers for disposal. Clean spillage area thoroughly with plenty of water.


	- Extinguishing media: Use extinguishing media appropriate to the surrounding fire conditions.

- Special hazards arising from the substance or mixture: Burning produces irritating, toxic and obnoxious fumes.

- Advice for firefighters: Wear suitable respiratory equipment when necessary.

	Handling and Storage
	Disposal Considerations

	- Precautions for safe handling: Avoid contact with eyes and skin. Ensure adequate ventilation of the working area. Adopt best

Manual Handling considerations when handling, carrying and dispensing.

- Conditions for safe storage, including any incompatibilities:
Keep in a cool, dry, well ventilated area. Keep containers tightly closed. Store in correctly labelled containers.
	Dispose of as special waste in compliance with local and national regulations.

	


	Assessor Summary
	
	YES/NO
	Further action

	1.
Has the assessment considered all factors 
pertinent to the use of the substance?  If NO 
please give 
details of further action required
	YES
	     

	2.
Has the assessment considered the 
practicability of preventing exposure?  If NO 
please give 
details of further action required
	YES
	     

	3.
Has the assessment considered the steps to 
be taken to achieve and maintain adequate 
control of exposure where prevention is not 
reasonably practicable?  If NO please give 
details of further action required
	YES
	     

	4.
Has the assessment considered the need for 
monitoring exposure to the substance  If NO 
please give details of further action required
	YES
	     

	5.
Has the assessment identified all action 
required to comply with regulations  If NO 
please give details of further action required
	YES
	     

	

	COSHH Assessment
	Please tick
	

	

	The task is safe to be carried out with current control procedures.
	X
	Tick if no further action required

	The task is safe to be carried out subject to actions listed
	     
	Tick if use of the substance is not causing significant problems but requires some action to bring it within COSHH guidelines, Action should be prioritised and specific dates set for completion

	Task/Substance is Unsafe, significant non-compliance with Health & Safety standards
	     
	Tick if the task or substance has potential to cause significant problems to users, use of substance to be discontinued until problems have been rectified
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