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	Name of Substance
	NO NONSENSE PVA
	COSHH

Reference 
	C049

	Supplied By
	Bostik Limited
	Date of 
Assessment
	25/07/25

	Persons at Risk
	Staff
       X
	Public          X
	
	Review Date
	24/07/26

	
	Visitors       X
	Contractor   X
	
	
	

	Description of Substance
	PVA Adhesive
	Method of use
	Apply directly on to the intended surface

	

	Hazards Identification and PPE

	Routes of Entry
	Personal Protective Equipment (Tick Required Boxes)
	Tick here for none
 FORMCHECKBOX 


	Inhalation
X
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	Absorption
X
	
	
	
	
	
	
	

	Ingestion
X
	
	
	
	
	
	
	

	Location
	Hand Protection
	Protective clothing
	Protective Footwear
	Safety Glasses
	Face Shield
	Face Mask
	Respirator

	     
	X
	X
	
	X
	
	
	X

	

	Risk Phrases

Safety Phrases
	Workplace exposure Limits (WEL) 

	P101 - If medical advice is needed, have product container or label at hand

P102 - Keep out of reach of children
	Type: Worker Long term Systemic health effects

Exposure route: Inhalation
Derived No Effect Level (DNEL) :17.6 mg/m³

Type: Worker Short term Systemic health effects

Exposure route: Inhalation

Derived No Effect Level (DNEL): 35.2 mg/m³

Type: Worker Long term Local health effects

Exposure route: Inhalation

Derived No Effect Level (DNEL) :17.6 mg/m³

Type: Worker Short term Local health effects

Exposure route: Inhalation

Derived No Effect Level (DNEL): 35.2 mg/m³

Type: Worker Long term Systemic health effects

Exposure route: Dermal

Derived No Effect Level (DNEL):  0.42 mg/kg bw/d

	

	Frequency & Duration of Exposure

	Amount Used

Small (Millilitres)
 X
Medium (Litres)
 FORMCHECKBOX 

Large (Cubic Metres)
 FORMCHECKBOX 

	How many times per day

1 – 5

 X
5 – 10

 FORMCHECKBOX 

More than 10
 FORMCHECKBOX 

	Duration

1 – 5 Minutes

 X
6 – 30 Minutes
 FORMCHECKBOX 

31 – 60 Minutes
 FORMCHECKBOX 
 
1 Hour & Above
 FORMCHECKBOX 


	SUBSTANCE PROPERTIES (Tick all that apply)
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	Oxidising
	Explosive
	Flammable
Highly Flammable
	Toxic
	Harmful or Irritant
	Corrosive
	Carcinogenic
Mutagenic
	Dangerous for environment

	
	
	
	
	X
	
	
	X


	GHS SUBSTANCE PROPERTIES
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	Oxidising
	Explosive
	(Extremely) Flammable
	Toxic
	Harmful
	Corrosive
	Human Health
	Dangerous for environment
	Gas under pressure

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	X
	 FORMCHECKBOX 



	Control Measures

	General Precautions
	First Aid Measures


	- General advice: Take a copy of the Safety Data Sheet when going for medical treatment.

- Inhalation: Remove to fresh air. IF exposed or concerned: Get medical advice/attention.

- Eye contact: Rinse thoroughly with plenty of water for at least 15 minutes, lifting lower and upper eyelids. Consult a doctor.

- Skin contact: Wash skin with soap and water. In the case of skin irritation or allergic reactions see a doctor.

- Ingestion: Clean mouth with water. Do NOT induce vomiting. Drink 1 or 2 glasses of water. Never give anything by mouth to an unconscious person.
     
	

	
	

	Further Controls Required
	Responsibility
	By When
	Date Done


	N/A 
	     
	     
	     

	

	Spillage Procedure
	Fire Prevention

	- Personal precautions: Ensure adequate ventilation. Avoid contact with skin, eyes or clothing.

- Other information: Ventilate the area. Prevent further leakage or spillage if safe to do so.
- Environmental precautions: Do not flush into surface water or sanitary sewer system. Do not allow to enter into soil/subsoil. See Section 12 for additional Ecological Information.
- Methods and material for containment and cleaning up: Use a non-combustible material like vermiculite, sand or earth to soak up the product and place into a container for later disposal.
- Methods for cleaning up: Take up mechanically, placing in appropriate containers for disposal.
	- Extinguishing media suitable extinguishing media: Use extinguishing measures that are appropriate to local circumstances and the surrounding environment.
- Unsuitable extinguishing media: Full water jet. Do not scatter spilled material with high pressure water streams.

- Special hazards arising from the substance or mixture specific hazards arising from the Chemical:

Thermal decomposition can lead to release of toxic and corrosive gases/vapours.

- Hazardous combustion products: Carbon monoxide. Carbon dioxide (CO2). Hydrocarbons.

- Advice for fire fighters special protective equipment for fire-fighters:
Firefighters should wear self-contained breathing apparatus and full firefighting turnout gear. Use personal protection equipment.


	Handling and Storage
	Disposal Considerations

	-  Precautions for safe handling: Advice on safe handling Ensure adequate ventilation. Use personal protective equipment as required. Avoid contact with skin, eyes or clothing.

- General hygiene considerations: Handle in accordance with good industrial hygiene and safety practice. Do not eat, drink or smoke when using this product. Wash thoroughly after handling. Take off all contaminated clothing and wash it before reuse.

- Storage Conditions: Keep container tightly closed in a dry and well-ventilated place. Keep away from food, drink and animal feeding stuffs.
	- Waste from residues/unused

Products: Dispose of contents/container in accordance with local, regional, national, and

international regulations as applicable.

- Contaminated packaging: Do not reuse empty containers. Handle contaminated packages in the same way as the product itself.

- Other information: Waste codes should be assigned by the user based on the application for which the product was used.

	


	Assessor Summary
	
	YES/NO
	Further action

	1.
Has the assessment considered all factors 
pertinent to the use of the substance?  If NO 
please give 
details of further action required
	YES
	     

	2.
Has the assessment considered the 
practicability of preventing exposure?  If NO 
please give 
details of further action required
	YES
	     

	3.
Has the assessment considered the steps to 
be taken to achieve and maintain adequate 
control of exposure where prevention is not 
reasonably practicable?  If NO please give 
details of further action required
	YES
	     

	4.
Has the assessment considered the need for 
monitoring exposure to the substance  If NO 
please give details of further action required
	YES
	     

	5.
Has the assessment identified all action 
required to comply with regulations  If NO 
please give details of further action required
	YES
	     

	

	COSHH Assessment
	Please tick
	

	

	The task is safe to be carried out with current control procedures.
	X
	Tick if no further action required

	The task is safe to be carried out subject to actions listed
	     
	Tick if use of the substance is not causing significant problems but requires some action to bring it within COSHH guidelines, Action should be prioritised and specific dates set for completion

	Task/Substance is Unsafe, significant non-compliance with Health & Safety standards
	     
	Tick if the task or substance has potential to cause significant problems to users, use of substance to be discontinued until problems have been rectified
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