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	Name of Substance
	UZIN PE 280
	COSHH

Reference
	C055

	Supplied

By
	Uzin
	Date of Assessment
	25/07/25

	Persons

at Risk
	Staff
	(
	Public
	
	Young
	
	Review

Date
	24/07/26

	
	Visitors
	(
	Contractors
	(
	Pregnant
	
	
	

	Description of Substance
	Film-Forming Dispersion Super-Fast Primer
	Method

of Use
	Used on existing surfaces requiring refurbishment, on well
bonded, waterproof residues of adhesives or levelling compounds (e.g. synthetic resin, neoprene, bitumen or

dispersion adhesives)


	Hazards Identification and PPE

	Routes of Entry
	Personal Protective Equipment Required (Tick as Appropriate)

	Inhalation
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	Absorption
	(
	
	
	
	
	
	
	

	Ingestion
	(
	Hand Protection
	Protective Clothing
	Protective Footwear
	Safety Glasses
	Face

Shield
	Face

Mask
	Respirator

	Comments:
	(
	
	
	
	
	
	

	
	
	
	
	
	
	
	


	Risk Phrases

Safety Phrases
	Occupational

Exposure Standard

(OES)
	Maximum

Exposure Limits

(MEL)
	Workplace

Exposure Limits

(WEL)

	N/A
	N/A
	N/A
	N/A


	Frequency & Duration Exposure

	Amount Used
	Home many times per day
	Duration

	Small (Millilitres)
	
	1-5
	(
	1-5 Minutes
	

	Medium (Litres)
	(
	5-10
	
	6-30 Minutes
	

	Large (Cubic Meters)
	
	More than 10
	
	31-60 Minutes
	

	
	1 Hour & Above
	(


	GHS Substance Properties
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	Oxidising
	Explosive
	(Extremely) Flammable
	Toxic
	Harmful
	Corrosive
	Human Health
	Dangerous for environment
	Gas under pressure

	
	
	
	
	
	
	
	
	


	Control Measures

	General Precautions
	First Aid Measures

	Solvent-free. Non-flammable. Requires no special protection or precautions in gen
eral use. Use of barrier cream and ventilation of the work area are recommended.

EMICODE EC 1 PLUS – very low emission. Within the scope of current knowledge,

gives off no emissions of formaldehyde, hazardous materials or volatile organic com
pounds (VOC). When fully dried, has a neutral odour and presents no physiological

or ecological risk. Basic prerequisites for best possible indoor air quality following

floor covering work are conformity to standards of the working conditions, as well as

thoroughly dry substrate, primer and smoothing compound.
	Skin Contact

Rinse with water. Contact physician if discomfort continues. Contact physician if irritation continues.

Eye Contact

Immediately flush with plenty of water. Remove any contact lenses and open eyes wide apart. Contact physician if irritation persists. Do not rub eye. 


	Further Controls Required
	Responsibility
	By When
	Completed

	N/A
	
	
	


	Spillage Procedure
	Fire Prevention

	Use mop or appropriate towel
	Product is non-combustible. Use fire extinguishing equipment appropriate for surrounding area.


	Handling and Storage
	Disposal Considerations

	Store in a dry place.
	Where possible, collect product residues and re-use. Do not allow dispersal into

drains, sewers or ground. Empty, scraped and drip-free plastic containers are recycla
ble. Containers with liquid residue, as well as the liquid product, are classed as Spe
cial Waste. Dried product residues are classed as Construction Waste.


	Assessor Summary
	YES / NO
	Further Action

	Has the assessment considered all factors pertinent to the use of the substance?

If NO please give details of further action required
	YES
	

	Has the assessment considered the practicability of preventing exposure?

If NO please give 
details of further action required
	YES
	

	Has the assessment considered the steps to 
be taken to achieve and maintain adequate control of exposure where prevention is not reasonably practicable?

If NO please give 
details of further action required
	YES
	

	Has the assessment considered the need for monitoring exposure to the substance?

If NO please give details of further action required
	YES
	

	Has the assessment identified all action required to comply with regulations?

If NO please give details of further action required
	YES
	


	COSHH Assessment

	The task is safe to be carried out with current control procedures.
	(
	No further action required

	The task is safe to be carried out subject to actions listed
	
	Use of the substance is not causing significant problems but requires some action to bring it within COSHH guidelines, Action should be prioritised and specific dates set for completion

	Task/Substance is Unsafe, significant non-compliance with Health & Safety standards
	
	Task or substance has potential to cause significant problems to users, use of substance to be discontinued until problems have been rectified
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